Partition Merge report for fpga_boot
Tue Jul 15 15:09:26 2025
Quartus II 64-Bit Version 13.0.0 Build 156 04/24/2013 SJ Full Version


---------------------
; Table of Contents ;
---------------------
  1. Legal Notice
  2. Partition Merge Summary
  3. Partition Merge Netlist Types Used
  4. Partition Merge Partition Warnings
  5. Partition Merge Partition Statistics
  6. Partition Merge Partition Pin Processing
  7. Partition Merge Resource Usage Summary
  8. Partition Merge Messages



----------------
; Legal Notice ;
----------------
Copyright (C) 1991-2013 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.



+----------------------------------------------------------------------------------+
; Partition Merge Summary                                                          ;
+------------------------------------+---------------------------------------------+
; Partition Merge Status             ; Successful - Tue Jul 15 15:09:26 2025       ;
; Quartus II 64-Bit Version          ; 13.0.0 Build 156 04/24/2013 SJ Full Version ;
; Revision Name                      ; fpga_boot                                   ;
; Top-level Entity Name              ; fpga_boot                                   ;
; Family                             ; Cyclone IV E                                ;
; Total logic elements               ; 33                                          ;
;     Total combinational functions  ; 32                                          ;
;     Dedicated logic registers      ; 1                                           ;
; Total registers                    ; 1                                           ;
; Total pins                         ; 9                                           ;
; Total virtual pins                 ; 1                                           ;
; Total memory bits                  ; 0                                           ;
; Embedded Multiplier 9-bit elements ; 0                                           ;
; Total PLLs                         ; 1                                           ;
+------------------------------------+---------------------------------------------+


+-------------------------------------------------------------------------------------------------------------------------------+
; Partition Merge Netlist Types Used                                                                                            ;
+--------------------------------+----------------+-------------------+------------------------+--------------------------------+
; Partition Name                 ; Partition Type ; Netlist Type Used ; Netlist Type Requested ; Partition Contents             ;
+--------------------------------+----------------+-------------------+------------------------+--------------------------------+
; Top                            ; User-created   ; Source File       ; Source File            ;                                ;
; rv32                           ; User-created   ; Source File       ; Source File            ; alta_rv32:rv32                 ;
; hard_block:auto_generated_inst ; Auto-generated ; Source File       ; Source File            ; hard_block:auto_generated_inst ;
+--------------------------------+----------------+-------------------+------------------------+--------------------------------+


+---------------------------------------------------------------------------+
; Partition Merge Partition Warnings                                        ;
+--------------------------------------+-----------+------------------------+
; Port                                 ; Partition ; Info                   ;
+--------------------------------------+-----------+------------------------+
; alta_rv32:rv32|ext_resetn            ; rv32      ; Driven by constant VCC ;
; alta_rv32:rv32|resetn_out            ; rv32      ; Driven by constant VCC ;
; alta_rv32:rv32|usb0_xcvr_clk         ; rv32      ; Driven by constant VCC ;
; alta_rv32:rv32|sys_ctrl_clkSource[0] ; rv32      ; Driven by constant VCC ;
; alta_rv32:rv32|usb0_id               ; rv32      ; Driven by constant VCC ;
; alta_rv32:rv32|slave_ahb_hready      ; rv32      ; Driven by constant VCC ;
; alta_rv32:rv32|mem_ahb_hreadyout     ; rv32      ; Driven by constant VCC ;
; alta_rv32:rv32|swj_JTAGIR[3]         ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|swj_JTAGIR[2]         ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|swj_JTAGIR[1]         ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|swj_JTAGIR[0]         ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|swj_JTAGSTATE[3]      ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|swj_JTAGSTATE[2]      ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|swj_JTAGSTATE[1]      ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|swj_JTAGSTATE[0]      ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|swj_JTAGNSW           ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|dmactive              ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio9_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio8_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio7_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio6_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio5_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio4_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio3_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio2_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio1_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_en[7]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_en[6]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_en[5]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_en[4]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_en[3]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_en[2]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_en[1]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_en[0]    ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_data[7]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_data[6]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_data[5]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_data[4]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_data[3]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_data[2]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_data[1]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|gpio0_io_out_data[0]  ; rv32      ; Driven by constant GND ;
; alta_rv32:rv32|sys_clk               ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hready        ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hreadyout     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_htrans[0]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_htrans[1]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hsize[0]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hsize[1]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hsize[2]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hburst[0]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hburst[1]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hburst[2]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwrite        ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[0]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[1]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[2]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[3]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[4]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[5]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[6]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[7]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[8]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[9]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[10]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[11]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[12]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[13]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[14]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[15]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[16]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[17]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[18]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[19]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[20]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[21]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[22]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[23]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[24]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[25]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[26]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[27]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[28]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[29]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[30]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_haddr[31]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[0]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[1]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[2]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[3]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[4]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[5]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[6]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[7]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[8]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[9]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[10]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[11]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[12]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[13]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[14]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[15]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[16]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[17]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[18]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[19]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[20]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[21]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[22]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[23]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[24]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[25]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[26]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[27]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[28]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[29]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[30]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|mem_ahb_hwdata[31]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hready      ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hreadyout   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_htrans[0]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_htrans[1]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hsize[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hsize[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hsize[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hburst[0]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hburst[1]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hburst[2]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwrite      ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[0]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[1]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[2]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[3]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[4]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[5]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[6]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[7]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[8]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[9]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[10]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[11]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[12]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[13]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[14]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[15]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[16]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[17]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[18]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[19]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[20]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[21]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[22]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[23]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[24]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[25]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[26]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[27]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[28]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[29]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[30]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hwdata[31]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hresp       ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[0]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[1]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[2]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[3]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[4]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[5]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[6]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[7]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[8]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[9]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[10]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[11]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[12]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[13]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[14]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[15]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[16]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[17]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[18]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[19]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[20]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[21]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[22]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[23]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[24]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[25]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[26]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[27]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[28]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[29]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[30]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|slave_ahb_hrdata[31]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_data[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_data[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_data[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_en[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_en[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_en[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio0_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_data[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_data[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_data[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_en[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_en[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_en[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio1_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|sys_ctrl_hseEnable    ; rv32      ; No fanout              ;
; alta_rv32:rv32|sys_ctrl_hseBypass    ; rv32      ; No fanout              ;
; alta_rv32:rv32|sys_ctrl_sleep        ; rv32      ; No fanout              ;
; alta_rv32:rv32|sys_ctrl_stop         ; rv32      ; No fanout              ;
; alta_rv32:rv32|sys_ctrl_standby      ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_data[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_data[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_data[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_en[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_en[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_en[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio2_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_data[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_data[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_data[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_en[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_en[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_en[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio3_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_data[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_data[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_data[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_en[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_en[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_en[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio4_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_data[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_data[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_data[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_en[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_en[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_en[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio5_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_data[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_en[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio6_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_data[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_data[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_data[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_en[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_en[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_en[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio7_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_data[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_data[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_data[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_en[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_en[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_en[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio8_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_in[0]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_in[1]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_in[2]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_in[3]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_in[4]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_in[5]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_in[6]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_in[7]        ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_data[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_data[4]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_data[5]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_data[6]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_data[7]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_en[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_en[4]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_en[5]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_en[6]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|gpio9_io_out_en[7]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|resetn_out            ; rv32      ; No fanout              ;
; alta_rv32:rv32|dmactive              ; rv32      ; No fanout              ;
; alta_rv32:rv32|swj_JTAGNSW           ; rv32      ; No fanout              ;
; alta_rv32:rv32|swj_JTAGSTATE[0]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|swj_JTAGSTATE[1]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|swj_JTAGSTATE[2]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|swj_JTAGSTATE[3]      ; rv32      ; No fanout              ;
; alta_rv32:rv32|swj_JTAGIR[0]         ; rv32      ; No fanout              ;
; alta_rv32:rv32|swj_JTAGIR[1]         ; rv32      ; No fanout              ;
; alta_rv32:rv32|swj_JTAGIR[2]         ; rv32      ; No fanout              ;
; alta_rv32:rv32|swj_JTAGIR[3]         ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_int[0]            ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_int[1]            ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_int[2]            ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_int[3]            ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_int[4]            ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_int[5]            ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_int[6]            ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_int[7]            ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACLBREQ[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACLBREQ[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACLBREQ[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACLBREQ[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACSREQ[0]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACSREQ[1]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACSREQ[2]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACSREQ[3]   ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACLSREQ[0]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACLSREQ[1]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACLSREQ[2]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACLSREQ[3]  ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACCLR[0]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACCLR[1]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACCLR[2]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACCLR[3]    ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACTC[0]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACTC[1]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACTC[2]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|ext_dma_DMACTC[3]     ; rv32      ; No fanout              ;
; alta_rv32:rv32|local_int[0]          ; rv32      ; No fanout              ;
; alta_rv32:rv32|local_int[1]          ; rv32      ; No fanout              ;
; alta_rv32:rv32|local_int[2]          ; rv32      ; No fanout              ;
; alta_rv32:rv32|local_int[3]          ; rv32      ; No fanout              ;
; alta_rv32:rv32|test_mode[0]          ; rv32      ; No fanout              ;
; alta_rv32:rv32|test_mode[1]          ; rv32      ; No fanout              ;
; alta_rv32:rv32|usb0_id               ; rv32      ; No fanout              ;
+--------------------------------------+-----------+------------------------+
Note: The Incremental Compilation Advisor can be used to get more detailed recommendations.


+-------------------------------------------------------------------------------------------+
; Partition Merge Partition Statistics                                                      ;
+---------------------------------------------+-----+------+--------------------------------+
; Statistic                                   ; Top ; rv32 ; hard_block:auto_generated_inst ;
+---------------------------------------------+-----+------+--------------------------------+
; Estimated Total logic elements              ; 32  ; 1    ; 0                              ;
;                                             ;     ;      ;                                ;
; Total combinational functions               ; 31  ; 1    ; 0                              ;
; Logic element usage by number of LUT inputs ;     ;      ;                                ;
;     -- 4 input functions                    ; 0   ; 0    ; 0                              ;
;     -- 3 input functions                    ; 0   ; 0    ; 0                              ;
;     -- <=2 input functions                  ; 31  ; 1    ; 0                              ;
;                                             ;     ;      ;                                ;
; Logic elements by mode                      ;     ;      ;                                ;
;     -- normal mode                          ; 31  ; 1    ; 0                              ;
;     -- arithmetic mode                      ; 0   ; 0    ; 0                              ;
;                                             ;     ;      ;                                ;
; Total registers                             ; 1   ; 0    ; 0                              ;
;     -- Dedicated logic registers            ; 1   ; 0    ; 0                              ;
;                                             ;     ;      ;                                ;
; Virtual pins                                ; 0   ; 1    ; 0                              ;
; I/O pins                                    ; 9   ; 0    ; 0                              ;
; Embedded Multiplier 9-bit elements          ; 0   ; 0    ; 0                              ;
; Total memory bits                           ; 0   ; 0    ; 0                              ;
; Total RAM block bits                        ; 0   ; 0    ; 0                              ;
; PLL                                         ; 0   ; 0    ; 1                              ;
;                                             ;     ;      ;                                ;
; Connections                                 ;     ;      ;                                ;
;     -- Input Connections                    ; 16  ; 1    ; 5                              ;
;     -- Registered Input Connections         ; 2   ; 0    ; 0                              ;
;     -- Output Connections                   ; 9   ; 10   ; 3                              ;
;     -- Registered Output Connections        ; 0   ; 0    ; 0                              ;
;                                             ;     ;      ;                                ;
; Internal Connections                        ;     ;      ;                                ;
;     -- Total Connections                    ; 43  ; 11   ; 10                             ;
;     -- Registered Connections               ; 2   ; 0    ; 0                              ;
;                                             ;     ;      ;                                ;
; External Connections                        ;     ;      ;                                ;
;     -- Top                                  ; 8   ; 10   ; 7                              ;
;     -- rv32                                 ; 10  ; 0    ; 1                              ;
;     -- hard_block:auto_generated_inst       ; 7   ; 1    ; 0                              ;
;                                             ;     ;      ;                                ;
; Partition Interface                         ;     ;      ;                                ;
;     -- Input Ports                          ; 4   ; 224  ; 5                              ;
;     -- Output Ports                         ; 4   ; 295  ; 2                              ;
;     -- Bidir Ports                          ; 1   ; 0    ; 0                              ;
;                                             ;     ;      ;                                ;
; Registered Ports                            ;     ;      ;                                ;
;     -- Registered Input Ports               ; 0   ; 0    ; 0                              ;
;     -- Registered Output Ports              ; 0   ; 0    ; 0                              ;
;                                             ;     ;      ;                                ;
; Port Connectivity                           ;     ;      ;                                ;
;     -- Input Ports driven by GND            ; 0   ; 215  ; 0                              ;
;     -- Output Ports driven by GND           ; 0   ; 170  ; 0                              ;
;     -- Input Ports driven by VCC            ; 0   ; 5    ; 0                              ;
;     -- Output Ports driven by VCC           ; 0   ; 0    ; 0                              ;
;     -- Input Ports with no Source           ; 0   ; 0    ; 0                              ;
;     -- Output Ports with no Source          ; 0   ; 0    ; 0                              ;
;     -- Input Ports with no Fanout           ; 0   ; 150  ; 0                              ;
;     -- Output Ports with no Fanout          ; 0   ; 282  ; 0                              ;
+---------------------------------------------+-----+------+--------------------------------+
Note: Resource usage numbers presented for Partitions containing post-synthesis logic are estimates.  For Partitions containing post-fit logic, resource usage numbers are accurate based on previous placement information.  Actual Fitter results may vary depending on current Fitter Preservation Level assignments.


+-----------------------------------------------------------------------------------------------------------+
; Partition Merge Partition Pin Processing                                                                  ;
+-----------------------+-----------+---------------+----------+--------------------------------------------+
; Name                  ; Partition ; Type          ; Location ; Status                                     ;
+-----------------------+-----------+---------------+----------+--------------------------------------------+
; GPIO3_0               ; Top       ; Input Port    ; n/a      ;                                            ;
;     -- GPIO3_0        ; Top       ; Input Pad     ; Unplaced ; Synthesized                                ;
;     -- GPIO3_0~input  ; Top       ; Input Buffer  ; Unplaced ; Synthesized                                ;
;                       ;           ;               ;          ;                                            ;
; GPIO6_0               ; Top       ; Output Port   ; n/a      ;                                            ;
;     -- GPIO6_0        ; Top       ; Output Pad    ; Unplaced ; Synthesized                                ;
;     -- GPIO6_0~output ; Top       ; Output Buffer ; Unplaced ; Preserved from Synthesis Netlist (WYSIWYG) ;
;                       ;           ;               ;          ;                                            ;
; GPIO6_2               ; Top       ; Output Port   ; n/a      ;                                            ;
;     -- GPIO6_2        ; Top       ; Output Pad    ; Unplaced ; Synthesized                                ;
;     -- GPIO6_2~output ; Top       ; Output Buffer ; Unplaced ; Preserved from Synthesis Netlist (WYSIWYG) ;
;                       ;           ;               ;          ;                                            ;
; GPIO9_0               ; Top       ; Output Port   ; n/a      ;                                            ;
;     -- GPIO9_0        ; Top       ; Output Pad    ; Unplaced ; Synthesized                                ;
;     -- GPIO9_0~output ; Top       ; Output Buffer ; Unplaced ; Preserved from Synthesis Netlist (WYSIWYG) ;
;                       ;           ;               ;          ;                                            ;
; GPIO9_1               ; Top       ; Bidir Port    ; n/a      ;                                            ;
;     -- GPIO9_1        ; Top       ; Bidir Pad     ; Unplaced ; Synthesized                                ;
;     -- GPIO9_1~output ; Top       ; Output Buffer ; Unplaced ; Preserved from Synthesis Netlist (WYSIWYG) ;
;                       ;           ;               ;          ;                                            ;
; GPIO9_2               ; Top       ; Output Port   ; n/a      ;                                            ;
;     -- GPIO9_2        ; Top       ; Output Pad    ; Unplaced ; Synthesized                                ;
;     -- GPIO9_2~output ; Top       ; Output Buffer ; Unplaced ; Preserved from Synthesis Netlist (WYSIWYG) ;
;                       ;           ;               ;          ;                                            ;
; PIN_HSE               ; Top       ; Input Port    ; n/a      ;                                            ;
;     -- PIN_HSE        ; Top       ; Input Pad     ; Unplaced ; Synthesized                                ;
;     -- PIN_HSE~input  ; Top       ; Input Buffer  ; Unplaced ; Synthesized                                ;
;                       ;           ;               ;          ;                                            ;
; PIN_HSI               ; Top       ; Input Port    ; n/a      ;                                            ;
;     -- PIN_HSI        ; Top       ; Input Pad     ; Unplaced ; Synthesized                                ;
;     -- PIN_HSI~input  ; Top       ; Input Buffer  ; Unplaced ; Synthesized                                ;
;                       ;           ;               ;          ;                                            ;
; PIN_OSC               ; Top       ; Input Port    ; n/a      ;                                            ;
;     -- PIN_OSC        ; Top       ; Input Pad     ; Unplaced ; Synthesized                                ;
;     -- PIN_OSC~input  ; Top       ; Input Buffer  ; Unplaced ; Synthesized                                ;
;                       ;           ;               ;          ;                                            ;
+-----------------------+-----------+---------------+----------+--------------------------------------------+


+-------------------------------------------------------------------+
; Partition Merge Resource Usage Summary                            ;
+---------------------------------------------+---------------------+
; Resource                                    ; Usage               ;
+---------------------------------------------+---------------------+
; Estimated Total logic elements              ; 33                  ;
;                                             ;                     ;
; Total combinational functions               ; 32                  ;
; Logic element usage by number of LUT inputs ;                     ;
;     -- 4 input functions                    ; 0                   ;
;     -- 3 input functions                    ; 0                   ;
;     -- <=2 input functions                  ; 32                  ;
;                                             ;                     ;
; Logic elements by mode                      ;                     ;
;     -- normal mode                          ; 32                  ;
;     -- arithmetic mode                      ; 0                   ;
;                                             ;                     ;
; Total registers                             ; 1                   ;
;     -- Dedicated logic registers            ; 1                   ;
;     -- I/O registers                        ; 0                   ;
;                                             ;                     ;
; Virtual pins                                ; 1                   ;
; I/O pins                                    ; 9                   ;
; Embedded Multiplier 9-bit elements          ; 0                   ;
; Total PLLs                                  ; 1                   ;
;     -- PLLs                                 ; 1                   ;
;                                             ;                     ;
; Maximum fan-out node                        ; alta_rv32:rv32|~GND ;
; Maximum fan-out                             ; 10                  ;
; Total fan-out                               ; 46                  ;
; Average fan-out                             ; 0.84                ;
+---------------------------------------------+---------------------+


+--------------------------+
; Partition Merge Messages ;
+--------------------------+
Info: *******************************************************************
Info: Running Quartus II 64-Bit Partition Merge
    Info: Version 13.0.0 Build 156 04/24/2013 SJ Full Version
    Info: Processing started: Tue Jul 15 15:09:25 2025
Info: Command: quartus_cdb --read_settings_files=off --write_settings_files=off fpga_boot -c fpga_boot --merge=on
Info (35007): Using synthesis netlist for partition "Top"
Info (35007): Using synthesis netlist for partition "rv32"
Info (35002): Resolved and merged 2 partition(s)
Info (16010): Generating hard_block partition "hard_block:auto_generated_inst"
    Info (16011): Adding 2 node(s), including 0 DDIO, 1 PLL, 0 transceiver and 0 LCELL
Info (35048): Found 177 ports with constant drivers. For more information, refer to the Partition Merger report
Info (35047): Found 433 ports with no fan-out. For more information, refer to the Partition Merger report
Warning (35016): Found partition port(s) not driving logic, possibly wasting area
    Warning (35017): Partition port "alta_rv32:rv32|sys_clk", driven by node "alta_gclksw:gclksw_inst|gclk_switch", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|sys_ctrl_standby", driven by node "altpll:pll_inst|altpll_9g32:auto_generated|locked", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|sys_ctrl_stop", driven by node "altpll:pll_inst|altpll_9g32:auto_generated|locked", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|sys_ctrl_sleep", driven by node "altpll:pll_inst|altpll_9g32:auto_generated|locked", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|sys_ctrl_hseBypass", driven by node "altpll:pll_inst|altpll_9g32:auto_generated|locked", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|sys_ctrl_hseEnable", driven by node "altpll:pll_inst|altpll_9g32:auto_generated|locked", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio3_io_in[0]", driven by node "gpio3_io_in[0]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio3_io_in[1]", driven by node "gpio3_io_in[1]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio3_io_in[2]", driven by node "gpio3_io_in[2]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio3_io_in[3]", driven by node "gpio3_io_in[3]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio3_io_in[4]", driven by node "gpio3_io_in[4]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio3_io_in[5]", driven by node "gpio3_io_in[5]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio3_io_in[6]", driven by node "gpio3_io_in[6]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio3_io_in[7]", driven by node "gpio3_io_in[7]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio9_io_in[0]", driven by node "gpio9_io_in[0]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio9_io_in[1]", driven by node "gpio9_io_in[1]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio9_io_in[2]", driven by node "gpio9_io_in[2]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio9_io_in[3]", driven by node "gpio9_io_in[3]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio9_io_in[4]", driven by node "gpio9_io_in[4]", does not drive logic
    Warning (35018): Partition port "alta_rv32:rv32|gpio9_io_in[5]", driven by node "gpio9_io_in[5]", does not drive logic
    Warning (35039): Only the first 20 ports are reported. For a full list of ports, refer to the Partition Warnings panel in the Partition Merge report
Warning (15899): PLL "altpll:pll_inst|altpll_9g32:auto_generated|pll1" has parameters clk1_multiply_by and clk1_divide_by specified but port CLK[1] is not connected
Warning (21074): Design contains 1 input pin(s) that do not drive logic
    Warning (15610): No output dependent on input pin "PIN_OSC"
Info (21057): Implemented 45 device resources after synthesis - the final resource count might be different
    Info (21058): Implemented 4 input pins
    Info (21059): Implemented 4 output pins
    Info (21060): Implemented 1 bidirectional pins
    Info (21061): Implemented 34 logic cells
    Info (21065): Implemented 1 PLLs
Info: Quartus II 64-Bit Partition Merge was successful. 0 errors, 25 warnings
    Info: Peak virtual memory: 4625 megabytes
    Info: Processing ended: Tue Jul 15 15:09:26 2025
    Info: Elapsed time: 00:00:01
    Info: Total CPU time (on all processors): 00:00:01


