// Copyright (C) 1991-2013 Altera Corporation
// Your use of Altera Corporation's design tools, logic functions 
// and other software and tools, and its AMPP partner logic 
// functions, and any output files from any of the foregoing 
// (including device programming or simulation files), and any 
// associated documentation or information are expressly subject 
// to the terms and conditions of the Altera Program License 
// Subscription Agreement, Altera MegaCore Function License 
// Agreement, or other applicable license agreement, including, 
// without limitation, that your use is for the sole purpose of 
// programming logic devices manufactured by Altera and sold by 
// Altera or its authorized distributors.  Please refer to the 
// applicable agreement for further details.

// VENDOR "Altera"
// PROGRAM "Quartus II 64-Bit"
// VERSION "Version 13.0.0 Build 156 04/24/2013 SJ Full Version"

// DATE "07/15/2025 15:09:48"

// 
// Device: Altera EP4CE75F29C8 Package FBGA780
// 

// 
// This Verilog file should be used for ModelSim (Verilog) only
// 

`timescale 1 ps/ 1 ps

module fpga_boot (
	GPIO3_0,
	GPIO6_0,
	GPIO6_2,
	GPIO9_0,
	GPIO9_1,
	GPIO9_2,
	PIN_HSE,
	PIN_HSI,
	PIN_OSC);
input 	GPIO3_0;
output 	GPIO6_0;
output 	GPIO6_2;
output 	GPIO9_0;
inout 	GPIO9_1;
output 	GPIO9_2;
input 	PIN_HSE;
input 	PIN_HSI;
input 	PIN_OSC;

// Design Ports Information
// GPIO6_0	=>  Location: PIN_AF14,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: 8mA
// GPIO6_2	=>  Location: PIN_AG12,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: 8mA
// GPIO9_0	=>  Location: PIN_AC15,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: 8mA
// GPIO9_2	=>  Location: PIN_AD15,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: 8mA
// PIN_OSC	=>  Location: PIN_AF13,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: Default
// GPIO9_1	=>  Location: PIN_AF15,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: 8mA
// GPIO3_0	=>  Location: PIN_AE13,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: Default
// PIN_HSI	=>  Location: PIN_Y2,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: Default
// PIN_HSE	=>  Location: PIN_J1,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: Default


wire gnd;
wire vcc;
wire unknown;

assign gnd = 1'b0;
assign vcc = 1'b1;
assign unknown = 1'bx;

tri1 devclrn;
tri1 devpor;
tri1 devoe;
// synopsys translate_off
initial $sdf_annotate("fpga_boot_8_1200mv_0c_v_slow.sdo");
// synopsys translate_on

wire \rv32.mem_ahb_hready ;
wire \rv32.mem_ahb_htrans[0] ;
wire \rv32.mem_ahb_htrans[1] ;
wire \rv32.mem_ahb_hsize[0] ;
wire \rv32.mem_ahb_hsize[1] ;
wire \rv32.mem_ahb_hsize[2] ;
wire \rv32.mem_ahb_hburst[0] ;
wire \rv32.mem_ahb_hburst[1] ;
wire \rv32.mem_ahb_hburst[2] ;
wire \rv32.mem_ahb_hwrite ;
wire \rv32.mem_ahb_haddr[0] ;
wire \rv32.mem_ahb_haddr[1] ;
wire \rv32.mem_ahb_haddr[2] ;
wire \rv32.mem_ahb_haddr[3] ;
wire \rv32.mem_ahb_haddr[4] ;
wire \rv32.mem_ahb_haddr[5] ;
wire \rv32.mem_ahb_haddr[6] ;
wire \rv32.mem_ahb_haddr[7] ;
wire \rv32.mem_ahb_haddr[8] ;
wire \rv32.mem_ahb_haddr[9] ;
wire \rv32.mem_ahb_haddr[10] ;
wire \rv32.mem_ahb_haddr[11] ;
wire \rv32.mem_ahb_haddr[12] ;
wire \rv32.mem_ahb_haddr[13] ;
wire \rv32.mem_ahb_haddr[14] ;
wire \rv32.mem_ahb_haddr[15] ;
wire \rv32.mem_ahb_haddr[16] ;
wire \rv32.mem_ahb_haddr[17] ;
wire \rv32.mem_ahb_haddr[18] ;
wire \rv32.mem_ahb_haddr[19] ;
wire \rv32.mem_ahb_haddr[20] ;
wire \rv32.mem_ahb_haddr[21] ;
wire \rv32.mem_ahb_haddr[22] ;
wire \rv32.mem_ahb_haddr[23] ;
wire \rv32.mem_ahb_haddr[24] ;
wire \rv32.mem_ahb_haddr[25] ;
wire \rv32.mem_ahb_haddr[26] ;
wire \rv32.mem_ahb_haddr[27] ;
wire \rv32.mem_ahb_haddr[28] ;
wire \rv32.mem_ahb_haddr[29] ;
wire \rv32.mem_ahb_haddr[30] ;
wire \rv32.mem_ahb_haddr[31] ;
wire \rv32.mem_ahb_hwdata[0] ;
wire \rv32.mem_ahb_hwdata[1] ;
wire \rv32.mem_ahb_hwdata[2] ;
wire \rv32.mem_ahb_hwdata[3] ;
wire \rv32.mem_ahb_hwdata[4] ;
wire \rv32.mem_ahb_hwdata[5] ;
wire \rv32.mem_ahb_hwdata[6] ;
wire \rv32.mem_ahb_hwdata[7] ;
wire \rv32.mem_ahb_hwdata[8] ;
wire \rv32.mem_ahb_hwdata[9] ;
wire \rv32.mem_ahb_hwdata[10] ;
wire \rv32.mem_ahb_hwdata[11] ;
wire \rv32.mem_ahb_hwdata[12] ;
wire \rv32.mem_ahb_hwdata[13] ;
wire \rv32.mem_ahb_hwdata[14] ;
wire \rv32.mem_ahb_hwdata[15] ;
wire \rv32.mem_ahb_hwdata[16] ;
wire \rv32.mem_ahb_hwdata[17] ;
wire \rv32.mem_ahb_hwdata[18] ;
wire \rv32.mem_ahb_hwdata[19] ;
wire \rv32.mem_ahb_hwdata[20] ;
wire \rv32.mem_ahb_hwdata[21] ;
wire \rv32.mem_ahb_hwdata[22] ;
wire \rv32.mem_ahb_hwdata[23] ;
wire \rv32.mem_ahb_hwdata[24] ;
wire \rv32.mem_ahb_hwdata[25] ;
wire \rv32.mem_ahb_hwdata[26] ;
wire \rv32.mem_ahb_hwdata[27] ;
wire \rv32.mem_ahb_hwdata[28] ;
wire \rv32.mem_ahb_hwdata[29] ;
wire \rv32.mem_ahb_hwdata[30] ;
wire \rv32.mem_ahb_hwdata[31] ;
wire \rv32.slave_ahb_hreadyout ;
wire \rv32.slave_ahb_hresp ;
wire \rv32.slave_ahb_hrdata[0] ;
wire \rv32.slave_ahb_hrdata[1] ;
wire \rv32.slave_ahb_hrdata[2] ;
wire \rv32.slave_ahb_hrdata[3] ;
wire \rv32.slave_ahb_hrdata[4] ;
wire \rv32.slave_ahb_hrdata[5] ;
wire \rv32.slave_ahb_hrdata[6] ;
wire \rv32.slave_ahb_hrdata[7] ;
wire \rv32.slave_ahb_hrdata[8] ;
wire \rv32.slave_ahb_hrdata[9] ;
wire \rv32.slave_ahb_hrdata[10] ;
wire \rv32.slave_ahb_hrdata[11] ;
wire \rv32.slave_ahb_hrdata[12] ;
wire \rv32.slave_ahb_hrdata[13] ;
wire \rv32.slave_ahb_hrdata[14] ;
wire \rv32.slave_ahb_hrdata[15] ;
wire \rv32.slave_ahb_hrdata[16] ;
wire \rv32.slave_ahb_hrdata[17] ;
wire \rv32.slave_ahb_hrdata[18] ;
wire \rv32.slave_ahb_hrdata[19] ;
wire \rv32.slave_ahb_hrdata[20] ;
wire \rv32.slave_ahb_hrdata[21] ;
wire \rv32.slave_ahb_hrdata[22] ;
wire \rv32.slave_ahb_hrdata[23] ;
wire \rv32.slave_ahb_hrdata[24] ;
wire \rv32.slave_ahb_hrdata[25] ;
wire \rv32.slave_ahb_hrdata[26] ;
wire \rv32.slave_ahb_hrdata[27] ;
wire \rv32.slave_ahb_hrdata[28] ;
wire \rv32.slave_ahb_hrdata[29] ;
wire \rv32.slave_ahb_hrdata[30] ;
wire \rv32.slave_ahb_hrdata[31] ;
wire \rv32.gpio0_io_out_data[0] ;
wire \rv32.gpio0_io_out_data[1] ;
wire \rv32.gpio0_io_out_data[2] ;
wire \rv32.gpio0_io_out_data[3] ;
wire \rv32.gpio0_io_out_data[4] ;
wire \rv32.gpio0_io_out_data[5] ;
wire \rv32.gpio0_io_out_data[6] ;
wire \rv32.gpio0_io_out_data[7] ;
wire \rv32.gpio0_io_out_en[0] ;
wire \rv32.gpio0_io_out_en[1] ;
wire \rv32.gpio0_io_out_en[2] ;
wire \rv32.gpio0_io_out_en[3] ;
wire \rv32.gpio0_io_out_en[4] ;
wire \rv32.gpio0_io_out_en[5] ;
wire \rv32.gpio0_io_out_en[6] ;
wire \rv32.gpio0_io_out_en[7] ;
wire \rv32.gpio1_io_out_data[0] ;
wire \rv32.gpio1_io_out_data[1] ;
wire \rv32.gpio1_io_out_data[2] ;
wire \rv32.gpio1_io_out_data[3] ;
wire \rv32.gpio1_io_out_data[4] ;
wire \rv32.gpio1_io_out_data[5] ;
wire \rv32.gpio1_io_out_data[6] ;
wire \rv32.gpio1_io_out_data[7] ;
wire \rv32.gpio1_io_out_en[0] ;
wire \rv32.gpio1_io_out_en[1] ;
wire \rv32.gpio1_io_out_en[2] ;
wire \rv32.gpio1_io_out_en[3] ;
wire \rv32.gpio1_io_out_en[4] ;
wire \rv32.gpio1_io_out_en[5] ;
wire \rv32.gpio1_io_out_en[6] ;
wire \rv32.gpio1_io_out_en[7] ;
wire \rv32.sys_ctrl_clkSource[0] ;
wire \rv32.sys_ctrl_clkSource[1] ;
wire \rv32.sys_ctrl_hseEnable ;
wire \rv32.sys_ctrl_hseBypass ;
wire \rv32.sys_ctrl_pllEnable ;
wire \rv32.sys_ctrl_sleep ;
wire \rv32.sys_ctrl_stop ;
wire \rv32.sys_ctrl_standby ;
wire \rv32.gpio2_io_out_data[0] ;
wire \rv32.gpio2_io_out_data[1] ;
wire \rv32.gpio2_io_out_data[2] ;
wire \rv32.gpio2_io_out_data[3] ;
wire \rv32.gpio2_io_out_data[4] ;
wire \rv32.gpio2_io_out_data[5] ;
wire \rv32.gpio2_io_out_data[6] ;
wire \rv32.gpio2_io_out_data[7] ;
wire \rv32.gpio2_io_out_en[0] ;
wire \rv32.gpio2_io_out_en[1] ;
wire \rv32.gpio2_io_out_en[2] ;
wire \rv32.gpio2_io_out_en[3] ;
wire \rv32.gpio2_io_out_en[4] ;
wire \rv32.gpio2_io_out_en[5] ;
wire \rv32.gpio2_io_out_en[6] ;
wire \rv32.gpio2_io_out_en[7] ;
wire \rv32.gpio3_io_out_data[0] ;
wire \rv32.gpio3_io_out_data[1] ;
wire \rv32.gpio3_io_out_data[2] ;
wire \rv32.gpio3_io_out_data[3] ;
wire \rv32.gpio3_io_out_data[4] ;
wire \rv32.gpio3_io_out_data[5] ;
wire \rv32.gpio3_io_out_data[6] ;
wire \rv32.gpio3_io_out_data[7] ;
wire \rv32.gpio3_io_out_en[0] ;
wire \rv32.gpio3_io_out_en[1] ;
wire \rv32.gpio3_io_out_en[2] ;
wire \rv32.gpio3_io_out_en[3] ;
wire \rv32.gpio3_io_out_en[4] ;
wire \rv32.gpio3_io_out_en[5] ;
wire \rv32.gpio3_io_out_en[6] ;
wire \rv32.gpio3_io_out_en[7] ;
wire \rv32.gpio4_io_out_data[0] ;
wire \rv32.gpio4_io_out_data[1] ;
wire \rv32.gpio4_io_out_data[2] ;
wire \rv32.gpio4_io_out_data[3] ;
wire \rv32.gpio4_io_out_data[4] ;
wire \rv32.gpio4_io_out_data[5] ;
wire \rv32.gpio4_io_out_data[6] ;
wire \rv32.gpio4_io_out_data[7] ;
wire \rv32.gpio4_io_out_en[0] ;
wire \rv32.gpio4_io_out_en[1] ;
wire \rv32.gpio4_io_out_en[2] ;
wire \rv32.gpio4_io_out_en[3] ;
wire \rv32.gpio4_io_out_en[4] ;
wire \rv32.gpio4_io_out_en[5] ;
wire \rv32.gpio4_io_out_en[6] ;
wire \rv32.gpio4_io_out_en[7] ;
wire \rv32.gpio5_io_out_data[0] ;
wire \rv32.gpio5_io_out_data[1] ;
wire \rv32.gpio5_io_out_data[2] ;
wire \rv32.gpio5_io_out_data[3] ;
wire \rv32.gpio5_io_out_data[4] ;
wire \rv32.gpio5_io_out_data[5] ;
wire \rv32.gpio5_io_out_data[6] ;
wire \rv32.gpio5_io_out_data[7] ;
wire \rv32.gpio5_io_out_en[0] ;
wire \rv32.gpio5_io_out_en[1] ;
wire \rv32.gpio5_io_out_en[2] ;
wire \rv32.gpio5_io_out_en[3] ;
wire \rv32.gpio5_io_out_en[4] ;
wire \rv32.gpio5_io_out_en[5] ;
wire \rv32.gpio5_io_out_en[6] ;
wire \rv32.gpio5_io_out_en[7] ;
wire \rv32.gpio6_io_out_data[0] ;
wire \rv32.gpio6_io_out_data[1] ;
wire \rv32.gpio6_io_out_data[2] ;
wire \rv32.gpio6_io_out_data[3] ;
wire \rv32.gpio6_io_out_data[4] ;
wire \rv32.gpio6_io_out_data[5] ;
wire \rv32.gpio6_io_out_data[6] ;
wire \rv32.gpio6_io_out_data[7] ;
wire \rv32.gpio6_io_out_en[0] ;
wire \rv32.gpio6_io_out_en[1] ;
wire \rv32.gpio6_io_out_en[2] ;
wire \rv32.gpio6_io_out_en[3] ;
wire \rv32.gpio6_io_out_en[4] ;
wire \rv32.gpio6_io_out_en[5] ;
wire \rv32.gpio6_io_out_en[6] ;
wire \rv32.gpio6_io_out_en[7] ;
wire \rv32.gpio7_io_out_data[0] ;
wire \rv32.gpio7_io_out_data[1] ;
wire \rv32.gpio7_io_out_data[2] ;
wire \rv32.gpio7_io_out_data[3] ;
wire \rv32.gpio7_io_out_data[4] ;
wire \rv32.gpio7_io_out_data[5] ;
wire \rv32.gpio7_io_out_data[6] ;
wire \rv32.gpio7_io_out_data[7] ;
wire \rv32.gpio7_io_out_en[0] ;
wire \rv32.gpio7_io_out_en[1] ;
wire \rv32.gpio7_io_out_en[2] ;
wire \rv32.gpio7_io_out_en[3] ;
wire \rv32.gpio7_io_out_en[4] ;
wire \rv32.gpio7_io_out_en[5] ;
wire \rv32.gpio7_io_out_en[6] ;
wire \rv32.gpio7_io_out_en[7] ;
wire \rv32.gpio8_io_out_data[0] ;
wire \rv32.gpio8_io_out_data[1] ;
wire \rv32.gpio8_io_out_data[2] ;
wire \rv32.gpio8_io_out_data[3] ;
wire \rv32.gpio8_io_out_data[4] ;
wire \rv32.gpio8_io_out_data[5] ;
wire \rv32.gpio8_io_out_data[6] ;
wire \rv32.gpio8_io_out_data[7] ;
wire \rv32.gpio8_io_out_en[0] ;
wire \rv32.gpio8_io_out_en[1] ;
wire \rv32.gpio8_io_out_en[2] ;
wire \rv32.gpio8_io_out_en[3] ;
wire \rv32.gpio8_io_out_en[4] ;
wire \rv32.gpio8_io_out_en[5] ;
wire \rv32.gpio8_io_out_en[6] ;
wire \rv32.gpio8_io_out_en[7] ;
wire \rv32.gpio9_io_out_data[0] ;
wire \rv32.gpio9_io_out_data[1] ;
wire \rv32.gpio9_io_out_data[2] ;
wire \rv32.gpio9_io_out_data[3] ;
wire \rv32.gpio9_io_out_data[4] ;
wire \rv32.gpio9_io_out_data[5] ;
wire \rv32.gpio9_io_out_data[6] ;
wire \rv32.gpio9_io_out_data[7] ;
wire \rv32.gpio9_io_out_en[0] ;
wire \rv32.gpio9_io_out_en[1] ;
wire \rv32.gpio9_io_out_en[2] ;
wire \rv32.gpio9_io_out_en[3] ;
wire \rv32.gpio9_io_out_en[4] ;
wire \rv32.gpio9_io_out_en[5] ;
wire \rv32.gpio9_io_out_en[6] ;
wire \rv32.gpio9_io_out_en[7] ;
wire \rv32.resetn_out ;
wire \rv32.dmactive ;
wire \rv32.swj_JTAGNSW ;
wire \rv32.swj_JTAGSTATE[0] ;
wire \rv32.swj_JTAGSTATE[1] ;
wire \rv32.swj_JTAGSTATE[2] ;
wire \rv32.swj_JTAGSTATE[3] ;
wire \rv32.swj_JTAGIR[0] ;
wire \rv32.swj_JTAGIR[1] ;
wire \rv32.swj_JTAGIR[2] ;
wire \rv32.swj_JTAGIR[3] ;
wire \rv32.ext_dma_DMACCLR[0] ;
wire \rv32.ext_dma_DMACCLR[1] ;
wire \rv32.ext_dma_DMACCLR[2] ;
wire \rv32.ext_dma_DMACCLR[3] ;
wire \rv32.ext_dma_DMACTC[0] ;
wire \rv32.ext_dma_DMACTC[1] ;
wire \rv32.ext_dma_DMACTC[2] ;
wire \rv32.ext_dma_DMACTC[3] ;
wire \auto_generated_inst.hbo_22_f9ff3d300b43c0f2_bp ;
wire \auto_generated_inst.hbo_13_1797ab7b230f061a_bp ;
wire \pll_inst|auto_generated|pll_lock_sync~q ;
wire \pll_inst|auto_generated|locked~combout ;
wire \~GND~combout ;
wire \~VCC~combout ;
wire \PIN_OSC~input_o ;
wire \GPIO9_1~input_o ;
wire \GPIO3_0~input_o ;
wire \PIN_HSI~input_o ;
wire \PIN_HSE~input_o ;
wire \pll_inst|auto_generated|locked~clkctrl_outclk ;
wire \pll_inst|auto_generated|pll_lock_sync~feeder_combout ;
wire \GPIO6_0~output_o ;
wire \GPIO6_2~output_o ;
wire \GPIO9_0~output_o ;
wire \GPIO9_2~output_o ;
wire \GPIO9_1~output_o ;
wire [7:0] gpio9_io_out_data;
wire [7:0] gpio6_io_out_en;
wire [7:0] gpio9_io_out_en;
wire [1:0] sys_ctrl_clkSource;
wire [7:0] gpio6_io_out_data;
wire [7:0] gpio9_io_in;
wire [7:0] gpio3_io_in;


alta_rv32 rv32(
	.sys_clk(\auto_generated_inst.hbo_22_f9ff3d300b43c0f2_bp ),
	.mem_ahb_hready(\rv32.mem_ahb_hready ),
	.mem_ahb_hreadyout(\~VCC~combout ),
	.mem_ahb_htrans({\rv32.mem_ahb_htrans[1] ,\rv32.mem_ahb_htrans[0] }),
	.mem_ahb_hsize({\rv32.mem_ahb_hsize[2] ,\rv32.mem_ahb_hsize[1] ,\rv32.mem_ahb_hsize[0] }),
	.mem_ahb_hburst({\rv32.mem_ahb_hburst[2] ,\rv32.mem_ahb_hburst[1] ,\rv32.mem_ahb_hburst[0] }),
	.mem_ahb_hwrite(\rv32.mem_ahb_hwrite ),
	.mem_ahb_haddr({\rv32.mem_ahb_haddr[31] ,\rv32.mem_ahb_haddr[30] ,\rv32.mem_ahb_haddr[29] ,\rv32.mem_ahb_haddr[28] ,\rv32.mem_ahb_haddr[27] ,\rv32.mem_ahb_haddr[26] ,\rv32.mem_ahb_haddr[25] ,\rv32.mem_ahb_haddr[24] ,\rv32.mem_ahb_haddr[23] ,\rv32.mem_ahb_haddr[22] ,
\rv32.mem_ahb_haddr[21] ,\rv32.mem_ahb_haddr[20] ,\rv32.mem_ahb_haddr[19] ,\rv32.mem_ahb_haddr[18] ,\rv32.mem_ahb_haddr[17] ,\rv32.mem_ahb_haddr[16] ,\rv32.mem_ahb_haddr[15] ,\rv32.mem_ahb_haddr[14] ,\rv32.mem_ahb_haddr[13] ,\rv32.mem_ahb_haddr[12] ,
\rv32.mem_ahb_haddr[11] ,\rv32.mem_ahb_haddr[10] ,\rv32.mem_ahb_haddr[9] ,\rv32.mem_ahb_haddr[8] ,\rv32.mem_ahb_haddr[7] ,\rv32.mem_ahb_haddr[6] ,\rv32.mem_ahb_haddr[5] ,\rv32.mem_ahb_haddr[4] ,\rv32.mem_ahb_haddr[3] ,\rv32.mem_ahb_haddr[2] ,\rv32.mem_ahb_haddr[1] ,
\rv32.mem_ahb_haddr[0] }),
	.mem_ahb_hwdata({\rv32.mem_ahb_hwdata[31] ,\rv32.mem_ahb_hwdata[30] ,\rv32.mem_ahb_hwdata[29] ,\rv32.mem_ahb_hwdata[28] ,\rv32.mem_ahb_hwdata[27] ,\rv32.mem_ahb_hwdata[26] ,\rv32.mem_ahb_hwdata[25] ,\rv32.mem_ahb_hwdata[24] ,\rv32.mem_ahb_hwdata[23] ,\rv32.mem_ahb_hwdata[22] ,
\rv32.mem_ahb_hwdata[21] ,\rv32.mem_ahb_hwdata[20] ,\rv32.mem_ahb_hwdata[19] ,\rv32.mem_ahb_hwdata[18] ,\rv32.mem_ahb_hwdata[17] ,\rv32.mem_ahb_hwdata[16] ,\rv32.mem_ahb_hwdata[15] ,\rv32.mem_ahb_hwdata[14] ,\rv32.mem_ahb_hwdata[13] ,\rv32.mem_ahb_hwdata[12] ,
\rv32.mem_ahb_hwdata[11] ,\rv32.mem_ahb_hwdata[10] ,\rv32.mem_ahb_hwdata[9] ,\rv32.mem_ahb_hwdata[8] ,\rv32.mem_ahb_hwdata[7] ,\rv32.mem_ahb_hwdata[6] ,\rv32.mem_ahb_hwdata[5] ,\rv32.mem_ahb_hwdata[4] ,\rv32.mem_ahb_hwdata[3] ,\rv32.mem_ahb_hwdata[2] ,
\rv32.mem_ahb_hwdata[1] ,\rv32.mem_ahb_hwdata[0] }),
	.mem_ahb_hresp(\~GND~combout ),
	.mem_ahb_hrdata({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,
\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.slave_ahb_hsel(\~GND~combout ),
	.slave_ahb_hready(\~VCC~combout ),
	.slave_ahb_hreadyout(\rv32.slave_ahb_hreadyout ),
	.slave_ahb_htrans({\~GND~combout ,\~GND~combout }),
	.slave_ahb_hsize({\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.slave_ahb_hburst({\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.slave_ahb_hwrite(\~GND~combout ),
	.slave_ahb_haddr({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,
\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.slave_ahb_hwdata({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,
\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.slave_ahb_hresp(\rv32.slave_ahb_hresp ),
	.slave_ahb_hrdata({\rv32.slave_ahb_hrdata[31] ,\rv32.slave_ahb_hrdata[30] ,\rv32.slave_ahb_hrdata[29] ,\rv32.slave_ahb_hrdata[28] ,\rv32.slave_ahb_hrdata[27] ,\rv32.slave_ahb_hrdata[26] ,\rv32.slave_ahb_hrdata[25] ,\rv32.slave_ahb_hrdata[24] ,\rv32.slave_ahb_hrdata[23] ,
\rv32.slave_ahb_hrdata[22] ,\rv32.slave_ahb_hrdata[21] ,\rv32.slave_ahb_hrdata[20] ,\rv32.slave_ahb_hrdata[19] ,\rv32.slave_ahb_hrdata[18] ,\rv32.slave_ahb_hrdata[17] ,\rv32.slave_ahb_hrdata[16] ,\rv32.slave_ahb_hrdata[15] ,\rv32.slave_ahb_hrdata[14] ,
\rv32.slave_ahb_hrdata[13] ,\rv32.slave_ahb_hrdata[12] ,\rv32.slave_ahb_hrdata[11] ,\rv32.slave_ahb_hrdata[10] ,\rv32.slave_ahb_hrdata[9] ,\rv32.slave_ahb_hrdata[8] ,\rv32.slave_ahb_hrdata[7] ,\rv32.slave_ahb_hrdata[6] ,\rv32.slave_ahb_hrdata[5] ,
\rv32.slave_ahb_hrdata[4] ,\rv32.slave_ahb_hrdata[3] ,\rv32.slave_ahb_hrdata[2] ,\rv32.slave_ahb_hrdata[1] ,\rv32.slave_ahb_hrdata[0] }),
	.gpio0_io_in({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.gpio0_io_out_data({\rv32.gpio0_io_out_data[7] ,\rv32.gpio0_io_out_data[6] ,\rv32.gpio0_io_out_data[5] ,\rv32.gpio0_io_out_data[4] ,\rv32.gpio0_io_out_data[3] ,\rv32.gpio0_io_out_data[2] ,\rv32.gpio0_io_out_data[1] ,\rv32.gpio0_io_out_data[0] }),
	.gpio0_io_out_en({\rv32.gpio0_io_out_en[7] ,\rv32.gpio0_io_out_en[6] ,\rv32.gpio0_io_out_en[5] ,\rv32.gpio0_io_out_en[4] ,\rv32.gpio0_io_out_en[3] ,\rv32.gpio0_io_out_en[2] ,\rv32.gpio0_io_out_en[1] ,\rv32.gpio0_io_out_en[0] }),
	.gpio1_io_in({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.gpio1_io_out_data({\rv32.gpio1_io_out_data[7] ,\rv32.gpio1_io_out_data[6] ,\rv32.gpio1_io_out_data[5] ,\rv32.gpio1_io_out_data[4] ,\rv32.gpio1_io_out_data[3] ,\rv32.gpio1_io_out_data[2] ,\rv32.gpio1_io_out_data[1] ,\rv32.gpio1_io_out_data[0] }),
	.gpio1_io_out_en({\rv32.gpio1_io_out_en[7] ,\rv32.gpio1_io_out_en[6] ,\rv32.gpio1_io_out_en[5] ,\rv32.gpio1_io_out_en[4] ,\rv32.gpio1_io_out_en[3] ,\rv32.gpio1_io_out_en[2] ,\rv32.gpio1_io_out_en[1] ,\rv32.gpio1_io_out_en[0] }),
	.sys_ctrl_clkSource({\rv32.sys_ctrl_clkSource[1] ,\rv32.sys_ctrl_clkSource[0] }),
	.sys_ctrl_hseEnable(\rv32.sys_ctrl_hseEnable ),
	.sys_ctrl_hseBypass(\rv32.sys_ctrl_hseBypass ),
	.sys_ctrl_pllEnable(\rv32.sys_ctrl_pllEnable ),
	.sys_ctrl_pllReady(\pll_inst|auto_generated|locked~combout ),
	.sys_ctrl_sleep(\rv32.sys_ctrl_sleep ),
	.sys_ctrl_stop(\rv32.sys_ctrl_stop ),
	.sys_ctrl_standby(\rv32.sys_ctrl_standby ),
	.gpio2_io_in({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.gpio2_io_out_data({\rv32.gpio2_io_out_data[7] ,\rv32.gpio2_io_out_data[6] ,\rv32.gpio2_io_out_data[5] ,\rv32.gpio2_io_out_data[4] ,\rv32.gpio2_io_out_data[3] ,\rv32.gpio2_io_out_data[2] ,\rv32.gpio2_io_out_data[1] ,\rv32.gpio2_io_out_data[0] }),
	.gpio2_io_out_en({\rv32.gpio2_io_out_en[7] ,\rv32.gpio2_io_out_en[6] ,\rv32.gpio2_io_out_en[5] ,\rv32.gpio2_io_out_en[4] ,\rv32.gpio2_io_out_en[3] ,\rv32.gpio2_io_out_en[2] ,\rv32.gpio2_io_out_en[1] ,\rv32.gpio2_io_out_en[0] }),
	.gpio3_io_in({gpio3_io_in[7],gpio3_io_in[6],gpio3_io_in[5],gpio3_io_in[4],gpio3_io_in[3],gpio3_io_in[2],gpio3_io_in[1],gpio3_io_in[0]}),
	.gpio3_io_out_data({\rv32.gpio3_io_out_data[7] ,\rv32.gpio3_io_out_data[6] ,\rv32.gpio3_io_out_data[5] ,\rv32.gpio3_io_out_data[4] ,\rv32.gpio3_io_out_data[3] ,\rv32.gpio3_io_out_data[2] ,\rv32.gpio3_io_out_data[1] ,\rv32.gpio3_io_out_data[0] }),
	.gpio3_io_out_en({\rv32.gpio3_io_out_en[7] ,\rv32.gpio3_io_out_en[6] ,\rv32.gpio3_io_out_en[5] ,\rv32.gpio3_io_out_en[4] ,\rv32.gpio3_io_out_en[3] ,\rv32.gpio3_io_out_en[2] ,\rv32.gpio3_io_out_en[1] ,\rv32.gpio3_io_out_en[0] }),
	.gpio4_io_in({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.gpio4_io_out_data({\rv32.gpio4_io_out_data[7] ,\rv32.gpio4_io_out_data[6] ,\rv32.gpio4_io_out_data[5] ,\rv32.gpio4_io_out_data[4] ,\rv32.gpio4_io_out_data[3] ,\rv32.gpio4_io_out_data[2] ,\rv32.gpio4_io_out_data[1] ,\rv32.gpio4_io_out_data[0] }),
	.gpio4_io_out_en({\rv32.gpio4_io_out_en[7] ,\rv32.gpio4_io_out_en[6] ,\rv32.gpio4_io_out_en[5] ,\rv32.gpio4_io_out_en[4] ,\rv32.gpio4_io_out_en[3] ,\rv32.gpio4_io_out_en[2] ,\rv32.gpio4_io_out_en[1] ,\rv32.gpio4_io_out_en[0] }),
	.gpio5_io_in({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.gpio5_io_out_data({\rv32.gpio5_io_out_data[7] ,\rv32.gpio5_io_out_data[6] ,\rv32.gpio5_io_out_data[5] ,\rv32.gpio5_io_out_data[4] ,\rv32.gpio5_io_out_data[3] ,\rv32.gpio5_io_out_data[2] ,\rv32.gpio5_io_out_data[1] ,\rv32.gpio5_io_out_data[0] }),
	.gpio5_io_out_en({\rv32.gpio5_io_out_en[7] ,\rv32.gpio5_io_out_en[6] ,\rv32.gpio5_io_out_en[5] ,\rv32.gpio5_io_out_en[4] ,\rv32.gpio5_io_out_en[3] ,\rv32.gpio5_io_out_en[2] ,\rv32.gpio5_io_out_en[1] ,\rv32.gpio5_io_out_en[0] }),
	.gpio6_io_in({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.gpio6_io_out_data({\rv32.gpio6_io_out_data[7] ,\rv32.gpio6_io_out_data[6] ,\rv32.gpio6_io_out_data[5] ,\rv32.gpio6_io_out_data[4] ,\rv32.gpio6_io_out_data[3] ,\rv32.gpio6_io_out_data[2] ,\rv32.gpio6_io_out_data[1] ,\rv32.gpio6_io_out_data[0] }),
	.gpio6_io_out_en({\rv32.gpio6_io_out_en[7] ,\rv32.gpio6_io_out_en[6] ,\rv32.gpio6_io_out_en[5] ,\rv32.gpio6_io_out_en[4] ,\rv32.gpio6_io_out_en[3] ,\rv32.gpio6_io_out_en[2] ,\rv32.gpio6_io_out_en[1] ,\rv32.gpio6_io_out_en[0] }),
	.gpio7_io_in({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.gpio7_io_out_data({\rv32.gpio7_io_out_data[7] ,\rv32.gpio7_io_out_data[6] ,\rv32.gpio7_io_out_data[5] ,\rv32.gpio7_io_out_data[4] ,\rv32.gpio7_io_out_data[3] ,\rv32.gpio7_io_out_data[2] ,\rv32.gpio7_io_out_data[1] ,\rv32.gpio7_io_out_data[0] }),
	.gpio7_io_out_en({\rv32.gpio7_io_out_en[7] ,\rv32.gpio7_io_out_en[6] ,\rv32.gpio7_io_out_en[5] ,\rv32.gpio7_io_out_en[4] ,\rv32.gpio7_io_out_en[3] ,\rv32.gpio7_io_out_en[2] ,\rv32.gpio7_io_out_en[1] ,\rv32.gpio7_io_out_en[0] }),
	.gpio8_io_in({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.gpio8_io_out_data({\rv32.gpio8_io_out_data[7] ,\rv32.gpio8_io_out_data[6] ,\rv32.gpio8_io_out_data[5] ,\rv32.gpio8_io_out_data[4] ,\rv32.gpio8_io_out_data[3] ,\rv32.gpio8_io_out_data[2] ,\rv32.gpio8_io_out_data[1] ,\rv32.gpio8_io_out_data[0] }),
	.gpio8_io_out_en({\rv32.gpio8_io_out_en[7] ,\rv32.gpio8_io_out_en[6] ,\rv32.gpio8_io_out_en[5] ,\rv32.gpio8_io_out_en[4] ,\rv32.gpio8_io_out_en[3] ,\rv32.gpio8_io_out_en[2] ,\rv32.gpio8_io_out_en[1] ,\rv32.gpio8_io_out_en[0] }),
	.gpio9_io_in({gpio9_io_in[7],gpio9_io_in[6],gpio9_io_in[5],gpio9_io_in[4],gpio9_io_in[3],gpio9_io_in[2],gpio9_io_in[1],gpio9_io_in[0]}),
	.gpio9_io_out_data({\rv32.gpio9_io_out_data[7] ,\rv32.gpio9_io_out_data[6] ,\rv32.gpio9_io_out_data[5] ,\rv32.gpio9_io_out_data[4] ,\rv32.gpio9_io_out_data[3] ,\rv32.gpio9_io_out_data[2] ,\rv32.gpio9_io_out_data[1] ,\rv32.gpio9_io_out_data[0] }),
	.gpio9_io_out_en({\rv32.gpio9_io_out_en[7] ,\rv32.gpio9_io_out_en[6] ,\rv32.gpio9_io_out_en[5] ,\rv32.gpio9_io_out_en[4] ,\rv32.gpio9_io_out_en[3] ,\rv32.gpio9_io_out_en[2] ,\rv32.gpio9_io_out_en[1] ,\rv32.gpio9_io_out_en[0] }),
	.ext_resetn(\~VCC~combout ),
	.resetn_out(\rv32.resetn_out ),
	.dmactive(\rv32.dmactive ),
	.swj_JTAGNSW(\rv32.swj_JTAGNSW ),
	.swj_JTAGSTATE({\rv32.swj_JTAGSTATE[3] ,\rv32.swj_JTAGSTATE[2] ,\rv32.swj_JTAGSTATE[1] ,\rv32.swj_JTAGSTATE[0] }),
	.swj_JTAGIR({\rv32.swj_JTAGIR[3] ,\rv32.swj_JTAGIR[2] ,\rv32.swj_JTAGIR[1] ,\rv32.swj_JTAGIR[0] }),
	.ext_int({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.ext_dma_DMACBREQ({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.ext_dma_DMACLBREQ({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.ext_dma_DMACSREQ({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.ext_dma_DMACLSREQ({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.ext_dma_DMACCLR({\rv32.ext_dma_DMACCLR[3] ,\rv32.ext_dma_DMACCLR[2] ,\rv32.ext_dma_DMACCLR[1] ,\rv32.ext_dma_DMACCLR[0] }),
	.ext_dma_DMACTC({\rv32.ext_dma_DMACTC[3] ,\rv32.ext_dma_DMACTC[2] ,\rv32.ext_dma_DMACTC[1] ,\rv32.ext_dma_DMACTC[0] }),
	.local_int({\~GND~combout ,\~GND~combout ,\~GND~combout ,\~GND~combout }),
	.test_mode({\~GND~combout ,\~GND~combout }),
	.usb0_xcvr_clk(\~VCC~combout ),
	.usb0_id(\~VCC~combout ),
	.devpor(devpor),
	.devclrn(devclrn),
	.devoe(devoe));

hard_block auto_generated_inst(
	.hbo_22_f9ff3d300b43c0f2_bp(\auto_generated_inst.hbo_22_f9ff3d300b43c0f2_bp ),
	.hbi_71_0_4730eacd893fc1ea_bp(\rv32.sys_ctrl_pllEnable ),
	.hbo_13_1797ab7b230f061a_bp(\auto_generated_inst.hbo_13_1797ab7b230f061a_bp ),
	.hbi_272_0_9cb2c0024f9919c5_bp(sys_ctrl_clkSource[0]),
	.hbi_272_1_9cb2c0024f9919c5_bp(sys_ctrl_clkSource[1]),
	.hbi_69_0_9cb2c0024f9919c5_bp(\PIN_HSI~input_o ),
	.hbi_7_0_4730eacd893fc1ea_bp(\PIN_HSE~input_o ),
	.devpor(devpor),
	.devclrn(devclrn),
	.devoe(devoe));

// Location: FF_X49_Y1_N1
dffeas \pll_inst|auto_generated|pll_lock_sync (
	.clk(\auto_generated_inst.hbo_13_1797ab7b230f061a_bp ),
	.d(\pll_inst|auto_generated|pll_lock_sync~feeder_combout ),
	.asdata(vcc),
	.clrn(\rv32.sys_ctrl_pllEnable ),
	.aload(gnd),
	.sclr(gnd),
	.sload(gnd),
	.ena(vcc),
	.devclrn(devclrn),
	.devpor(devpor),
	.q(\pll_inst|auto_generated|pll_lock_sync~q ),
	.prn(vcc));
// synopsys translate_off
defparam \pll_inst|auto_generated|pll_lock_sync .is_wysiwyg = "true";
defparam \pll_inst|auto_generated|pll_lock_sync .power_up = "low";
// synopsys translate_on

// Location: LCCOMB_X49_Y1_N26
cycloneive_lcell_comb \pll_inst|auto_generated|locked (
// Equation(s):
// \pll_inst|auto_generated|locked~combout  = (\pll_inst|auto_generated|pll1~LOCKED  & \pll_inst|auto_generated|pll_lock_sync~q )

	.dataa(gnd),
	.datab(gnd),
	.datac(\auto_generated_inst.hbo_13_1797ab7b230f061a_bp ),
	.datad(\pll_inst|auto_generated|pll_lock_sync~q ),
	.cin(gnd),
	.combout(\pll_inst|auto_generated|locked~combout ),
	.cout());
// synopsys translate_off
defparam \pll_inst|auto_generated|locked .lut_mask = 16'hF000;
defparam \pll_inst|auto_generated|locked .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X57_Y5_N0
cycloneive_lcell_comb \sys_ctrl_clkSource[0] (
// Equation(s):
// sys_ctrl_clkSource[0] = LCELL(\~VCC~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(\rv32.sys_ctrl_clkSource[0] ),
	.cin(gnd),
	.combout(sys_ctrl_clkSource[0]),
	.cout());
// synopsys translate_off
defparam \sys_ctrl_clkSource[0] .lut_mask = 16'hFF00;
defparam \sys_ctrl_clkSource[0] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X57_Y5_N2
cycloneive_lcell_comb \sys_ctrl_clkSource[1] (
// Equation(s):
// sys_ctrl_clkSource[1] = LCELL(\pll_inst|auto_generated|locked~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(\rv32.sys_ctrl_clkSource[1] ),
	.datad(gnd),
	.cin(gnd),
	.combout(sys_ctrl_clkSource[1]),
	.cout());
// synopsys translate_off
defparam \sys_ctrl_clkSource[1] .lut_mask = 16'hF0F0;
defparam \sys_ctrl_clkSource[1] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X57_Y5_N10
cycloneive_lcell_comb \~VCC (
// Equation(s):
// \~VCC~combout  = VCC

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(\~VCC~combout ),
	.cout());
// synopsys translate_off
defparam \~VCC .lut_mask = 16'hFFFF;
defparam \~VCC .sum_lutc_input = "datac";
// synopsys translate_on

// Location: IOIBUF_X51_Y0_N1
cycloneive_io_ibuf \GPIO9_1~input (
	.i(GPIO9_1),
	.ibar(gnd),
	.o(\GPIO9_1~input_o ));
// synopsys translate_off
defparam \GPIO9_1~input .bus_hold = "false";
defparam \GPIO9_1~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X43_Y0_N8
cycloneive_io_ibuf \GPIO3_0~input (
	.i(GPIO3_0),
	.ibar(gnd),
	.o(\GPIO3_0~input_o ));
// synopsys translate_off
defparam \GPIO3_0~input .bus_hold = "false";
defparam \GPIO3_0~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X0_Y30_N15
cycloneive_io_ibuf \PIN_HSI~input (
	.i(PIN_HSI),
	.ibar(gnd),
	.o(\PIN_HSI~input_o ));
// synopsys translate_off
defparam \PIN_HSI~input .bus_hold = "false";
defparam \PIN_HSI~input .simulate_z_as = "z";
// synopsys translate_on

// Location: IOIBUF_X0_Y30_N8
cycloneive_io_ibuf \PIN_HSE~input (
	.i(PIN_HSE),
	.ibar(gnd),
	.o(\PIN_HSE~input_o ));
// synopsys translate_off
defparam \PIN_HSE~input .bus_hold = "false";
defparam \PIN_HSE~input .simulate_z_as = "z";
// synopsys translate_on

// Location: CLKCTRL_G16
cycloneive_clkctrl \pll_inst|auto_generated|locked~clkctrl (
	.ena(vcc),
	.inclk({vcc,vcc,vcc,\pll_inst|auto_generated|locked~combout }),
	.clkselect(2'b00),
	.devclrn(devclrn),
	.devpor(devpor),
	.outclk(\pll_inst|auto_generated|locked~clkctrl_outclk ));
// synopsys translate_off
defparam \pll_inst|auto_generated|locked~clkctrl .clock_type = "global clock";
defparam \pll_inst|auto_generated|locked~clkctrl .ena_register_mode = "none";
// synopsys translate_on

// Location: LCCOMB_X49_Y1_N0
cycloneive_lcell_comb \pll_inst|auto_generated|pll_lock_sync~feeder (
// Equation(s):
// \pll_inst|auto_generated|pll_lock_sync~feeder_combout  = VCC

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(\pll_inst|auto_generated|pll_lock_sync~feeder_combout ),
	.cout());
// synopsys translate_off
defparam \pll_inst|auto_generated|pll_lock_sync~feeder .lut_mask = 16'hFFFF;
defparam \pll_inst|auto_generated|pll_lock_sync~feeder .sum_lutc_input = "datac";
// synopsys translate_on

// Location: IOOBUF_X47_Y0_N16
cycloneive_io_obuf \GPIO6_0~output (
	.i(gpio6_io_out_data[0]),
	.oe(gpio6_io_out_en[0]),
	.seriesterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(\GPIO6_0~output_o ),
	.obar());
// synopsys translate_off
defparam \GPIO6_0~output .bus_hold = "false";
defparam \GPIO6_0~output .open_drain_output = "false";
// synopsys translate_on

// Location: IOOBUF_X47_Y0_N9
cycloneive_io_obuf \GPIO6_2~output (
	.i(gpio6_io_out_data[2]),
	.oe(gpio6_io_out_en[2]),
	.seriesterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(\GPIO6_2~output_o ),
	.obar());
// synopsys translate_off
defparam \GPIO6_2~output .bus_hold = "false";
defparam \GPIO6_2~output .open_drain_output = "false";
// synopsys translate_on

// Location: IOOBUF_X51_Y0_N23
cycloneive_io_obuf \GPIO9_0~output (
	.i(gpio9_io_out_data[0]),
	.oe(gpio9_io_out_en[0]),
	.seriesterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(\GPIO9_0~output_o ),
	.obar());
// synopsys translate_off
defparam \GPIO9_0~output .bus_hold = "false";
defparam \GPIO9_0~output .open_drain_output = "false";
// synopsys translate_on

// Location: IOOBUF_X51_Y0_N16
cycloneive_io_obuf \GPIO9_2~output (
	.i(gpio9_io_out_data[2]),
	.oe(gpio9_io_out_en[2]),
	.seriesterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(\GPIO9_2~output_o ),
	.obar());
// synopsys translate_off
defparam \GPIO9_2~output .bus_hold = "false";
defparam \GPIO9_2~output .open_drain_output = "false";
// synopsys translate_on

// Location: IOOBUF_X51_Y0_N2
cycloneive_io_obuf \GPIO9_1~output (
	.i(gpio9_io_out_data[1]),
	.oe(gpio9_io_out_en[1]),
	.seriesterminationcontrol(16'b0000000000000000),
	.devoe(devoe),
	.o(\GPIO9_1~output_o ),
	.obar());
// synopsys translate_off
defparam \GPIO9_1~output .bus_hold = "false";
defparam \GPIO9_1~output .open_drain_output = "false";
// synopsys translate_on

// Location: LCCOMB_X47_Y4_N26
cycloneive_lcell_comb \gpio6_io_out_data[0] (
// Equation(s):
// gpio6_io_out_data[0] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(\rv32.gpio6_io_out_data[0] ),
	.cin(gnd),
	.combout(gpio6_io_out_data[0]),
	.cout());
// synopsys translate_off
defparam \gpio6_io_out_data[0] .lut_mask = 16'hFF00;
defparam \gpio6_io_out_data[0] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X48_Y4_N20
cycloneive_lcell_comb \gpio6_io_out_en[0] (
// Equation(s):
// gpio6_io_out_en[0] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(\rv32.gpio6_io_out_en[0] ),
	.cin(gnd),
	.combout(gpio6_io_out_en[0]),
	.cout());
// synopsys translate_off
defparam \gpio6_io_out_en[0] .lut_mask = 16'hFF00;
defparam \gpio6_io_out_en[0] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X47_Y4_N30
cycloneive_lcell_comb \gpio6_io_out_data[2] (
// Equation(s):
// gpio6_io_out_data[2] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(\rv32.gpio6_io_out_data[2] ),
	.cin(gnd),
	.combout(gpio6_io_out_data[2]),
	.cout());
// synopsys translate_off
defparam \gpio6_io_out_data[2] .lut_mask = 16'hFF00;
defparam \gpio6_io_out_data[2] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X48_Y4_N24
cycloneive_lcell_comb \gpio6_io_out_en[2] (
// Equation(s):
// gpio6_io_out_en[2] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(\rv32.gpio6_io_out_en[2] ),
	.cin(gnd),
	.combout(gpio6_io_out_en[2]),
	.cout());
// synopsys translate_off
defparam \gpio6_io_out_en[2] .lut_mask = 16'hFF00;
defparam \gpio6_io_out_en[2] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X51_Y3_N2
cycloneive_lcell_comb \gpio9_io_out_data[0] (
// Equation(s):
// gpio9_io_out_data[0] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(\rv32.gpio9_io_out_data[0] ),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_out_data[0]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_out_data[0] .lut_mask = 16'hF0F0;
defparam \gpio9_io_out_data[0] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X52_Y4_N26
cycloneive_lcell_comb \gpio9_io_out_en[0] (
// Equation(s):
// gpio9_io_out_en[0] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(\rv32.gpio9_io_out_en[0] ),
	.cin(gnd),
	.combout(gpio9_io_out_en[0]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_out_en[0] .lut_mask = 16'hFF00;
defparam \gpio9_io_out_en[0] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X51_Y3_N6
cycloneive_lcell_comb \gpio9_io_out_data[2] (
// Equation(s):
// gpio9_io_out_data[2] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(\rv32.gpio9_io_out_data[2] ),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_out_data[2]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_out_data[2] .lut_mask = 16'hF0F0;
defparam \gpio9_io_out_data[2] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X52_Y4_N30
cycloneive_lcell_comb \gpio9_io_out_en[2] (
// Equation(s):
// gpio9_io_out_en[2] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(\rv32.gpio9_io_out_en[2] ),
	.cin(gnd),
	.combout(gpio9_io_out_en[2]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_out_en[2] .lut_mask = 16'hFF00;
defparam \gpio9_io_out_en[2] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X51_Y3_N4
cycloneive_lcell_comb \gpio9_io_out_data[1] (
// Equation(s):
// gpio9_io_out_data[1] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(\rv32.gpio9_io_out_data[1] ),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_out_data[1]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_out_data[1] .lut_mask = 16'hF0F0;
defparam \gpio9_io_out_data[1] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X52_Y4_N28
cycloneive_lcell_comb \gpio9_io_out_en[1] (
// Equation(s):
// gpio9_io_out_en[1] = LCELL(\~GND~combout )

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(\rv32.gpio9_io_out_en[1] ),
	.cin(gnd),
	.combout(gpio9_io_out_en[1]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_out_en[1] .lut_mask = 16'hFF00;
defparam \gpio9_io_out_en[1] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X44_Y4_N0
cycloneive_lcell_comb \gpio3_io_in[0] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(\GPIO3_0~input_o ),
	.cin(gnd),
	.combout(gpio3_io_in[0]),
	.cout());
// synopsys translate_off
defparam \gpio3_io_in[0] .lut_mask = 16'hFF00;
defparam \gpio3_io_in[0] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X44_Y4_N2
cycloneive_lcell_comb \gpio3_io_in[1] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio3_io_in[1]),
	.cout());
// synopsys translate_off
defparam \gpio3_io_in[1] .lut_mask = 16'h0000;
defparam \gpio3_io_in[1] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X44_Y4_N4
cycloneive_lcell_comb \gpio3_io_in[2] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio3_io_in[2]),
	.cout());
// synopsys translate_off
defparam \gpio3_io_in[2] .lut_mask = 16'h0000;
defparam \gpio3_io_in[2] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X44_Y4_N6
cycloneive_lcell_comb \gpio3_io_in[3] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio3_io_in[3]),
	.cout());
// synopsys translate_off
defparam \gpio3_io_in[3] .lut_mask = 16'h0000;
defparam \gpio3_io_in[3] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X44_Y4_N8
cycloneive_lcell_comb \gpio3_io_in[4] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio3_io_in[4]),
	.cout());
// synopsys translate_off
defparam \gpio3_io_in[4] .lut_mask = 16'h0000;
defparam \gpio3_io_in[4] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X44_Y4_N10
cycloneive_lcell_comb \gpio3_io_in[5] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio3_io_in[5]),
	.cout());
// synopsys translate_off
defparam \gpio3_io_in[5] .lut_mask = 16'h0000;
defparam \gpio3_io_in[5] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X44_Y4_N12
cycloneive_lcell_comb \gpio3_io_in[6] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio3_io_in[6]),
	.cout());
// synopsys translate_off
defparam \gpio3_io_in[6] .lut_mask = 16'h0000;
defparam \gpio3_io_in[6] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X44_Y4_N14
cycloneive_lcell_comb \gpio3_io_in[7] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio3_io_in[7]),
	.cout());
// synopsys translate_off
defparam \gpio3_io_in[7] .lut_mask = 16'h0000;
defparam \gpio3_io_in[7] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X50_Y4_N0
cycloneive_lcell_comb \gpio9_io_in[0] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_in[0]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_in[0] .lut_mask = 16'h0000;
defparam \gpio9_io_in[0] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X50_Y4_N2
cycloneive_lcell_comb \gpio9_io_in[1] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(\GPIO9_1~input_o ),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_in[1]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_in[1] .lut_mask = 16'hF0F0;
defparam \gpio9_io_in[1] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X50_Y4_N4
cycloneive_lcell_comb \gpio9_io_in[2] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_in[2]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_in[2] .lut_mask = 16'h0000;
defparam \gpio9_io_in[2] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X50_Y4_N6
cycloneive_lcell_comb \gpio9_io_in[3] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_in[3]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_in[3] .lut_mask = 16'h0000;
defparam \gpio9_io_in[3] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X50_Y4_N8
cycloneive_lcell_comb \gpio9_io_in[4] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_in[4]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_in[4] .lut_mask = 16'h0000;
defparam \gpio9_io_in[4] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X50_Y4_N10
cycloneive_lcell_comb \gpio9_io_in[5] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_in[5]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_in[5] .lut_mask = 16'h0000;
defparam \gpio9_io_in[5] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X50_Y4_N12
cycloneive_lcell_comb \gpio9_io_in[6] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_in[6]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_in[6] .lut_mask = 16'h0000;
defparam \gpio9_io_in[6] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X50_Y4_N14
cycloneive_lcell_comb \gpio9_io_in[7] (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(gpio9_io_in[7]),
	.cout());
// synopsys translate_off
defparam \gpio9_io_in[7] .lut_mask = 16'h0000;
defparam \gpio9_io_in[7] .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X57_Y9_N0
cycloneive_lcell_comb \~GND (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(\~GND~combout ),
	.cout());
// synopsys translate_off
defparam \~GND .lut_mask = 16'h0000;
defparam \~GND .sum_lutc_input = "datac";
// synopsys translate_on

// Location: IOIBUF_X43_Y0_N1
cycloneive_io_ibuf \PIN_OSC~input (
	.i(PIN_OSC),
	.ibar(gnd),
	.o(\PIN_OSC~input_o ));
// synopsys translate_off
defparam \PIN_OSC~input .bus_hold = "false";
defparam \PIN_OSC~input .simulate_z_as = "z";
// synopsys translate_on

assign GPIO6_0 = \GPIO6_0~output_o ;

assign GPIO6_2 = \GPIO6_2~output_o ;

assign GPIO9_0 = \GPIO9_0~output_o ;

assign GPIO9_2 = \GPIO9_2~output_o ;

assign GPIO9_1 = \GPIO9_1~output_o ;

endmodule

module alta_rv32 (
	sys_clk,
	mem_ahb_hready,
	mem_ahb_hreadyout,
	mem_ahb_htrans,
	mem_ahb_hsize,
	mem_ahb_hburst,
	mem_ahb_hwrite,
	mem_ahb_haddr,
	mem_ahb_hwdata,
	mem_ahb_hresp,
	mem_ahb_hrdata,
	slave_ahb_hsel,
	slave_ahb_hready,
	slave_ahb_hreadyout,
	slave_ahb_htrans,
	slave_ahb_hsize,
	slave_ahb_hburst,
	slave_ahb_hwrite,
	slave_ahb_haddr,
	slave_ahb_hwdata,
	slave_ahb_hresp,
	slave_ahb_hrdata,
	gpio0_io_in,
	gpio0_io_out_data,
	gpio0_io_out_en,
	gpio1_io_in,
	gpio1_io_out_data,
	gpio1_io_out_en,
	sys_ctrl_clkSource,
	sys_ctrl_hseEnable,
	sys_ctrl_hseBypass,
	sys_ctrl_pllEnable,
	sys_ctrl_pllReady,
	sys_ctrl_sleep,
	sys_ctrl_stop,
	sys_ctrl_standby,
	gpio2_io_in,
	gpio2_io_out_data,
	gpio2_io_out_en,
	gpio3_io_in,
	gpio3_io_out_data,
	gpio3_io_out_en,
	gpio4_io_in,
	gpio4_io_out_data,
	gpio4_io_out_en,
	gpio5_io_in,
	gpio5_io_out_data,
	gpio5_io_out_en,
	gpio6_io_in,
	gpio6_io_out_data,
	gpio6_io_out_en,
	gpio7_io_in,
	gpio7_io_out_data,
	gpio7_io_out_en,
	gpio8_io_in,
	gpio8_io_out_data,
	gpio8_io_out_en,
	gpio9_io_in,
	gpio9_io_out_data,
	gpio9_io_out_en,
	ext_resetn,
	resetn_out,
	dmactive,
	swj_JTAGNSW,
	swj_JTAGSTATE,
	swj_JTAGIR,
	ext_int,
	ext_dma_DMACBREQ,
	ext_dma_DMACLBREQ,
	ext_dma_DMACSREQ,
	ext_dma_DMACLSREQ,
	ext_dma_DMACCLR,
	ext_dma_DMACTC,
	local_int,
	test_mode,
	usb0_xcvr_clk,
	usb0_id,
	devpor,
	devclrn,
	devoe);
input 	sys_clk;
output 	mem_ahb_hready;
input 	mem_ahb_hreadyout;
output 	[1:0] mem_ahb_htrans;
output 	[2:0] mem_ahb_hsize;
output 	[2:0] mem_ahb_hburst;
output 	mem_ahb_hwrite;
output 	[31:0] mem_ahb_haddr;
output 	[31:0] mem_ahb_hwdata;
input 	mem_ahb_hresp;
input 	[31:0] mem_ahb_hrdata;
input 	slave_ahb_hsel;
input 	slave_ahb_hready;
output 	slave_ahb_hreadyout;
input 	[1:0] slave_ahb_htrans;
input 	[2:0] slave_ahb_hsize;
input 	[2:0] slave_ahb_hburst;
input 	slave_ahb_hwrite;
input 	[31:0] slave_ahb_haddr;
input 	[31:0] slave_ahb_hwdata;
output 	slave_ahb_hresp;
output 	[31:0] slave_ahb_hrdata;
input 	[7:0] gpio0_io_in;
output 	[7:0] gpio0_io_out_data;
output 	[7:0] gpio0_io_out_en;
input 	[7:0] gpio1_io_in;
output 	[7:0] gpio1_io_out_data;
output 	[7:0] gpio1_io_out_en;
output 	[1:0] sys_ctrl_clkSource;
output 	sys_ctrl_hseEnable;
output 	sys_ctrl_hseBypass;
output 	sys_ctrl_pllEnable;
input 	sys_ctrl_pllReady;
output 	sys_ctrl_sleep;
output 	sys_ctrl_stop;
output 	sys_ctrl_standby;
input 	[7:0] gpio2_io_in;
output 	[7:0] gpio2_io_out_data;
output 	[7:0] gpio2_io_out_en;
input 	[7:0] gpio3_io_in;
output 	[7:0] gpio3_io_out_data;
output 	[7:0] gpio3_io_out_en;
input 	[7:0] gpio4_io_in;
output 	[7:0] gpio4_io_out_data;
output 	[7:0] gpio4_io_out_en;
input 	[7:0] gpio5_io_in;
output 	[7:0] gpio5_io_out_data;
output 	[7:0] gpio5_io_out_en;
input 	[7:0] gpio6_io_in;
output 	[7:0] gpio6_io_out_data;
output 	[7:0] gpio6_io_out_en;
input 	[7:0] gpio7_io_in;
output 	[7:0] gpio7_io_out_data;
output 	[7:0] gpio7_io_out_en;
input 	[7:0] gpio8_io_in;
output 	[7:0] gpio8_io_out_data;
output 	[7:0] gpio8_io_out_en;
input 	[7:0] gpio9_io_in;
output 	[7:0] gpio9_io_out_data;
output 	[7:0] gpio9_io_out_en;
input 	ext_resetn;
output 	resetn_out;
output 	dmactive;
output 	swj_JTAGNSW;
output 	[3:0] swj_JTAGSTATE;
output 	[3:0] swj_JTAGIR;
input 	[7:0] ext_int;
input 	[3:0] ext_dma_DMACBREQ;
input 	[3:0] ext_dma_DMACLBREQ;
input 	[3:0] ext_dma_DMACSREQ;
input 	[3:0] ext_dma_DMACLSREQ;
output 	[3:0] ext_dma_DMACCLR;
output 	[3:0] ext_dma_DMACTC;
input 	[3:0] local_int;
input 	[1:0] test_mode;
input 	usb0_xcvr_clk;
input 	usb0_id;

// Design Ports Information

input 	devpor;
input 	devclrn;
input 	devoe;

wire gnd;
wire vcc;
wire unknown;

assign gnd = 1'b0;
assign vcc = 1'b1;
assign unknown = 1'bx;

wire \~GND~combout ;
wire \sys_clk~QIC_DANGLING_PORT_combout ;


// Location: LCCOMB_X50_Y3_N0
cycloneive_lcell_comb \~GND (
// Equation(s):
// \~GND~combout  = GND

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(gnd),
	.cin(gnd),
	.combout(\~GND~combout ),
	.cout());
// synopsys translate_off
defparam \~GND .lut_mask = 16'h0000;
defparam \~GND .sum_lutc_input = "datac";
// synopsys translate_on

// Location: LCCOMB_X46_Y3_N0
cycloneive_lcell_comb \sys_clk~QIC_DANGLING_PORT (
// Equation(s):

	.dataa(gnd),
	.datab(gnd),
	.datac(gnd),
	.datad(sys_clk),
	.cin(gnd),
	.combout(\sys_clk~QIC_DANGLING_PORT_combout ),
	.cout());
// synopsys translate_off
defparam \sys_clk~QIC_DANGLING_PORT .lut_mask = 16'hFF00;
defparam \sys_clk~QIC_DANGLING_PORT .sum_lutc_input = "datac";
// synopsys translate_on

assign mem_ahb_hready = mem_ahb_hresp;

assign mem_ahb_htrans[0] = mem_ahb_hresp;

assign mem_ahb_htrans[1] = mem_ahb_hresp;

assign mem_ahb_hsize[0] = mem_ahb_hresp;

assign mem_ahb_hsize[1] = mem_ahb_hresp;

assign mem_ahb_hsize[2] = mem_ahb_hresp;

assign mem_ahb_hburst[0] = mem_ahb_hresp;

assign mem_ahb_hburst[1] = mem_ahb_hresp;

assign mem_ahb_hburst[2] = mem_ahb_hresp;

assign mem_ahb_hwrite = mem_ahb_hresp;

assign mem_ahb_haddr[0] = mem_ahb_hrdata[0];

assign mem_ahb_haddr[1] = mem_ahb_hrdata[1];

assign mem_ahb_haddr[2] = mem_ahb_hrdata[2];

assign mem_ahb_haddr[3] = mem_ahb_hrdata[3];

assign mem_ahb_haddr[4] = mem_ahb_hrdata[4];

assign mem_ahb_haddr[5] = mem_ahb_hrdata[5];

assign mem_ahb_haddr[6] = mem_ahb_hrdata[6];

assign mem_ahb_haddr[7] = mem_ahb_hrdata[7];

assign mem_ahb_haddr[8] = mem_ahb_hrdata[8];

assign mem_ahb_haddr[9] = mem_ahb_hrdata[9];

assign mem_ahb_haddr[10] = mem_ahb_hrdata[10];

assign mem_ahb_haddr[11] = mem_ahb_hrdata[11];

assign mem_ahb_haddr[12] = mem_ahb_hrdata[12];

assign mem_ahb_haddr[13] = mem_ahb_hrdata[13];

assign mem_ahb_haddr[14] = mem_ahb_hrdata[14];

assign mem_ahb_haddr[15] = mem_ahb_hrdata[15];

assign mem_ahb_haddr[16] = mem_ahb_hrdata[16];

assign mem_ahb_haddr[17] = mem_ahb_hrdata[17];

assign mem_ahb_haddr[18] = mem_ahb_hrdata[18];

assign mem_ahb_haddr[19] = mem_ahb_hrdata[19];

assign mem_ahb_haddr[20] = mem_ahb_hrdata[20];

assign mem_ahb_haddr[21] = mem_ahb_hrdata[21];

assign mem_ahb_haddr[22] = mem_ahb_hrdata[22];

assign mem_ahb_haddr[23] = mem_ahb_hrdata[23];

assign mem_ahb_haddr[24] = mem_ahb_hrdata[24];

assign mem_ahb_haddr[25] = mem_ahb_hrdata[25];

assign mem_ahb_haddr[26] = mem_ahb_hrdata[26];

assign mem_ahb_haddr[27] = mem_ahb_hrdata[27];

assign mem_ahb_haddr[28] = mem_ahb_hrdata[28];

assign mem_ahb_haddr[29] = mem_ahb_hrdata[29];

assign mem_ahb_haddr[30] = mem_ahb_hrdata[30];

assign mem_ahb_haddr[31] = mem_ahb_hrdata[31];

assign mem_ahb_hwdata[0] = mem_ahb_hrdata[0];

assign mem_ahb_hwdata[1] = mem_ahb_hrdata[1];

assign mem_ahb_hwdata[2] = mem_ahb_hrdata[2];

assign mem_ahb_hwdata[3] = mem_ahb_hrdata[3];

assign mem_ahb_hwdata[4] = mem_ahb_hrdata[4];

assign mem_ahb_hwdata[5] = mem_ahb_hrdata[5];

assign mem_ahb_hwdata[6] = mem_ahb_hrdata[6];

assign mem_ahb_hwdata[7] = mem_ahb_hrdata[7];

assign mem_ahb_hwdata[8] = mem_ahb_hrdata[8];

assign mem_ahb_hwdata[9] = mem_ahb_hrdata[9];

assign mem_ahb_hwdata[10] = mem_ahb_hrdata[10];

assign mem_ahb_hwdata[11] = mem_ahb_hrdata[11];

assign mem_ahb_hwdata[12] = mem_ahb_hrdata[12];

assign mem_ahb_hwdata[13] = mem_ahb_hrdata[13];

assign mem_ahb_hwdata[14] = mem_ahb_hrdata[14];

assign mem_ahb_hwdata[15] = mem_ahb_hrdata[15];

assign mem_ahb_hwdata[16] = mem_ahb_hrdata[16];

assign mem_ahb_hwdata[17] = mem_ahb_hrdata[17];

assign mem_ahb_hwdata[18] = mem_ahb_hrdata[18];

assign mem_ahb_hwdata[19] = mem_ahb_hrdata[19];

assign mem_ahb_hwdata[20] = mem_ahb_hrdata[20];

assign mem_ahb_hwdata[21] = mem_ahb_hrdata[21];

assign mem_ahb_hwdata[22] = mem_ahb_hrdata[22];

assign mem_ahb_hwdata[23] = mem_ahb_hrdata[23];

assign mem_ahb_hwdata[24] = mem_ahb_hrdata[24];

assign mem_ahb_hwdata[25] = mem_ahb_hrdata[25];

assign mem_ahb_hwdata[26] = mem_ahb_hrdata[26];

assign mem_ahb_hwdata[27] = mem_ahb_hrdata[27];

assign mem_ahb_hwdata[28] = mem_ahb_hrdata[28];

assign mem_ahb_hwdata[29] = mem_ahb_hrdata[29];

assign mem_ahb_hwdata[30] = mem_ahb_hrdata[30];

assign mem_ahb_hwdata[31] = mem_ahb_hrdata[31];

assign slave_ahb_hreadyout = slave_ahb_hsel;

assign slave_ahb_hresp = slave_ahb_hsel;

assign slave_ahb_hrdata[0] = slave_ahb_haddr[0];

assign slave_ahb_hrdata[1] = slave_ahb_haddr[1];

assign slave_ahb_hrdata[2] = slave_ahb_haddr[2];

assign slave_ahb_hrdata[3] = slave_ahb_haddr[3];

assign slave_ahb_hrdata[4] = slave_ahb_haddr[4];

assign slave_ahb_hrdata[5] = slave_ahb_haddr[5];

assign slave_ahb_hrdata[6] = slave_ahb_haddr[6];

assign slave_ahb_hrdata[7] = slave_ahb_haddr[7];

assign slave_ahb_hrdata[8] = slave_ahb_haddr[8];

assign slave_ahb_hrdata[9] = slave_ahb_haddr[9];

assign slave_ahb_hrdata[10] = slave_ahb_haddr[10];

assign slave_ahb_hrdata[11] = slave_ahb_haddr[11];

assign slave_ahb_hrdata[12] = slave_ahb_haddr[12];

assign slave_ahb_hrdata[13] = slave_ahb_haddr[13];

assign slave_ahb_hrdata[14] = slave_ahb_haddr[14];

assign slave_ahb_hrdata[15] = slave_ahb_haddr[15];

assign slave_ahb_hrdata[16] = slave_ahb_haddr[16];

assign slave_ahb_hrdata[17] = slave_ahb_haddr[17];

assign slave_ahb_hrdata[18] = slave_ahb_haddr[18];

assign slave_ahb_hrdata[19] = slave_ahb_haddr[19];

assign slave_ahb_hrdata[20] = slave_ahb_haddr[20];

assign slave_ahb_hrdata[21] = slave_ahb_haddr[21];

assign slave_ahb_hrdata[22] = slave_ahb_haddr[22];

assign slave_ahb_hrdata[23] = slave_ahb_haddr[23];

assign slave_ahb_hrdata[24] = slave_ahb_haddr[24];

assign slave_ahb_hrdata[25] = slave_ahb_haddr[25];

assign slave_ahb_hrdata[26] = slave_ahb_haddr[26];

assign slave_ahb_hrdata[27] = slave_ahb_haddr[27];

assign slave_ahb_hrdata[28] = slave_ahb_haddr[28];

assign slave_ahb_hrdata[29] = slave_ahb_haddr[29];

assign slave_ahb_hrdata[30] = slave_ahb_haddr[30];

assign slave_ahb_hrdata[31] = slave_ahb_haddr[31];

assign gpio0_io_out_data[0] = \~GND~combout ;

assign gpio0_io_out_data[1] = \~GND~combout ;

assign gpio0_io_out_data[2] = \~GND~combout ;

assign gpio0_io_out_data[3] = \~GND~combout ;

assign gpio0_io_out_data[4] = \~GND~combout ;

assign gpio0_io_out_data[5] = \~GND~combout ;

assign gpio0_io_out_data[6] = \~GND~combout ;

assign gpio0_io_out_data[7] = \~GND~combout ;

assign gpio0_io_out_en[0] = \~GND~combout ;

assign gpio0_io_out_en[1] = \~GND~combout ;

assign gpio0_io_out_en[2] = \~GND~combout ;

assign gpio0_io_out_en[3] = \~GND~combout ;

assign gpio0_io_out_en[4] = \~GND~combout ;

assign gpio0_io_out_en[5] = \~GND~combout ;

assign gpio0_io_out_en[6] = \~GND~combout ;

assign gpio0_io_out_en[7] = \~GND~combout ;

assign gpio1_io_out_data[0] = \~GND~combout ;

assign gpio1_io_out_data[1] = \~GND~combout ;

assign gpio1_io_out_data[2] = \~GND~combout ;

assign gpio1_io_out_data[3] = \~GND~combout ;

assign gpio1_io_out_data[4] = \~GND~combout ;

assign gpio1_io_out_data[5] = \~GND~combout ;

assign gpio1_io_out_data[6] = \~GND~combout ;

assign gpio1_io_out_data[7] = \~GND~combout ;

assign gpio1_io_out_en[0] = \~GND~combout ;

assign gpio1_io_out_en[1] = \~GND~combout ;

assign gpio1_io_out_en[2] = \~GND~combout ;

assign gpio1_io_out_en[3] = \~GND~combout ;

assign gpio1_io_out_en[4] = \~GND~combout ;

assign gpio1_io_out_en[5] = \~GND~combout ;

assign gpio1_io_out_en[6] = \~GND~combout ;

assign gpio1_io_out_en[7] = \~GND~combout ;

assign sys_ctrl_clkSource[0] = usb0_xcvr_clk;

assign sys_ctrl_clkSource[1] = sys_ctrl_pllReady;

assign sys_ctrl_hseEnable = sys_ctrl_pllReady;

assign sys_ctrl_hseBypass = sys_ctrl_pllReady;

assign sys_ctrl_pllEnable = sys_ctrl_pllReady;

assign sys_ctrl_sleep = sys_ctrl_pllReady;

assign sys_ctrl_stop = sys_ctrl_pllReady;

assign sys_ctrl_standby = sys_ctrl_pllReady;

assign gpio2_io_out_data[0] = \~GND~combout ;

assign gpio2_io_out_data[1] = \~GND~combout ;

assign gpio2_io_out_data[2] = \~GND~combout ;

assign gpio2_io_out_data[3] = \~GND~combout ;

assign gpio2_io_out_data[4] = \~GND~combout ;

assign gpio2_io_out_data[5] = \~GND~combout ;

assign gpio2_io_out_data[6] = \~GND~combout ;

assign gpio2_io_out_data[7] = \~GND~combout ;

assign gpio2_io_out_en[0] = \~GND~combout ;

assign gpio2_io_out_en[1] = \~GND~combout ;

assign gpio2_io_out_en[2] = \~GND~combout ;

assign gpio2_io_out_en[3] = \~GND~combout ;

assign gpio2_io_out_en[4] = \~GND~combout ;

assign gpio2_io_out_en[5] = \~GND~combout ;

assign gpio2_io_out_en[6] = \~GND~combout ;

assign gpio2_io_out_en[7] = \~GND~combout ;

assign gpio3_io_out_data[0] = \~GND~combout ;

assign gpio3_io_out_data[1] = \~GND~combout ;

assign gpio3_io_out_data[2] = \~GND~combout ;

assign gpio3_io_out_data[3] = \~GND~combout ;

assign gpio3_io_out_data[4] = \~GND~combout ;

assign gpio3_io_out_data[5] = \~GND~combout ;

assign gpio3_io_out_data[6] = \~GND~combout ;

assign gpio3_io_out_data[7] = \~GND~combout ;

assign gpio3_io_out_en[0] = \~GND~combout ;

assign gpio3_io_out_en[1] = \~GND~combout ;

assign gpio3_io_out_en[2] = \~GND~combout ;

assign gpio3_io_out_en[3] = \~GND~combout ;

assign gpio3_io_out_en[4] = \~GND~combout ;

assign gpio3_io_out_en[5] = \~GND~combout ;

assign gpio3_io_out_en[6] = \~GND~combout ;

assign gpio3_io_out_en[7] = \~GND~combout ;

assign gpio4_io_out_data[0] = \~GND~combout ;

assign gpio4_io_out_data[1] = \~GND~combout ;

assign gpio4_io_out_data[2] = \~GND~combout ;

assign gpio4_io_out_data[3] = \~GND~combout ;

assign gpio4_io_out_data[4] = \~GND~combout ;

assign gpio4_io_out_data[5] = \~GND~combout ;

assign gpio4_io_out_data[6] = \~GND~combout ;

assign gpio4_io_out_data[7] = \~GND~combout ;

assign gpio4_io_out_en[0] = \~GND~combout ;

assign gpio4_io_out_en[1] = \~GND~combout ;

assign gpio4_io_out_en[2] = \~GND~combout ;

assign gpio4_io_out_en[3] = \~GND~combout ;

assign gpio4_io_out_en[4] = \~GND~combout ;

assign gpio4_io_out_en[5] = \~GND~combout ;

assign gpio4_io_out_en[6] = \~GND~combout ;

assign gpio4_io_out_en[7] = \~GND~combout ;

assign gpio5_io_out_data[0] = \~GND~combout ;

assign gpio5_io_out_data[1] = \~GND~combout ;

assign gpio5_io_out_data[2] = \~GND~combout ;

assign gpio5_io_out_data[3] = \~GND~combout ;

assign gpio5_io_out_data[4] = \~GND~combout ;

assign gpio5_io_out_data[5] = \~GND~combout ;

assign gpio5_io_out_data[6] = \~GND~combout ;

assign gpio5_io_out_data[7] = \~GND~combout ;

assign gpio5_io_out_en[0] = \~GND~combout ;

assign gpio5_io_out_en[1] = \~GND~combout ;

assign gpio5_io_out_en[2] = \~GND~combout ;

assign gpio5_io_out_en[3] = \~GND~combout ;

assign gpio5_io_out_en[4] = \~GND~combout ;

assign gpio5_io_out_en[5] = \~GND~combout ;

assign gpio5_io_out_en[6] = \~GND~combout ;

assign gpio5_io_out_en[7] = \~GND~combout ;

assign gpio6_io_out_data[0] = \~GND~combout ;

assign gpio6_io_out_data[1] = \~GND~combout ;

assign gpio6_io_out_data[2] = \~GND~combout ;

assign gpio6_io_out_data[3] = \~GND~combout ;

assign gpio6_io_out_data[4] = \~GND~combout ;

assign gpio6_io_out_data[5] = \~GND~combout ;

assign gpio6_io_out_data[6] = \~GND~combout ;

assign gpio6_io_out_data[7] = \~GND~combout ;

assign gpio6_io_out_en[0] = \~GND~combout ;

assign gpio6_io_out_en[1] = \~GND~combout ;

assign gpio6_io_out_en[2] = \~GND~combout ;

assign gpio6_io_out_en[3] = \~GND~combout ;

assign gpio6_io_out_en[4] = \~GND~combout ;

assign gpio6_io_out_en[5] = \~GND~combout ;

assign gpio6_io_out_en[6] = \~GND~combout ;

assign gpio6_io_out_en[7] = \~GND~combout ;

assign gpio7_io_out_data[0] = \~GND~combout ;

assign gpio7_io_out_data[1] = \~GND~combout ;

assign gpio7_io_out_data[2] = \~GND~combout ;

assign gpio7_io_out_data[3] = \~GND~combout ;

assign gpio7_io_out_data[4] = \~GND~combout ;

assign gpio7_io_out_data[5] = \~GND~combout ;

assign gpio7_io_out_data[6] = \~GND~combout ;

assign gpio7_io_out_data[7] = \~GND~combout ;

assign gpio7_io_out_en[0] = \~GND~combout ;

assign gpio7_io_out_en[1] = \~GND~combout ;

assign gpio7_io_out_en[2] = \~GND~combout ;

assign gpio7_io_out_en[3] = \~GND~combout ;

assign gpio7_io_out_en[4] = \~GND~combout ;

assign gpio7_io_out_en[5] = \~GND~combout ;

assign gpio7_io_out_en[6] = \~GND~combout ;

assign gpio7_io_out_en[7] = \~GND~combout ;

assign gpio8_io_out_data[0] = \~GND~combout ;

assign gpio8_io_out_data[1] = \~GND~combout ;

assign gpio8_io_out_data[2] = \~GND~combout ;

assign gpio8_io_out_data[3] = \~GND~combout ;

assign gpio8_io_out_data[4] = \~GND~combout ;

assign gpio8_io_out_data[5] = \~GND~combout ;

assign gpio8_io_out_data[6] = \~GND~combout ;

assign gpio8_io_out_data[7] = \~GND~combout ;

assign gpio8_io_out_en[0] = \~GND~combout ;

assign gpio8_io_out_en[1] = \~GND~combout ;

assign gpio8_io_out_en[2] = \~GND~combout ;

assign gpio8_io_out_en[3] = \~GND~combout ;

assign gpio8_io_out_en[4] = \~GND~combout ;

assign gpio8_io_out_en[5] = \~GND~combout ;

assign gpio8_io_out_en[6] = \~GND~combout ;

assign gpio8_io_out_en[7] = \~GND~combout ;

assign gpio9_io_out_data[0] = \~GND~combout ;

assign gpio9_io_out_data[1] = \~GND~combout ;

assign gpio9_io_out_data[2] = \~GND~combout ;

assign gpio9_io_out_data[3] = \~GND~combout ;

assign gpio9_io_out_data[4] = \~GND~combout ;

assign gpio9_io_out_data[5] = \~GND~combout ;

assign gpio9_io_out_data[6] = \~GND~combout ;

assign gpio9_io_out_data[7] = \~GND~combout ;

assign gpio9_io_out_en[0] = \~GND~combout ;

assign gpio9_io_out_en[1] = \~GND~combout ;

assign gpio9_io_out_en[2] = \~GND~combout ;

assign gpio9_io_out_en[3] = \~GND~combout ;

assign gpio9_io_out_en[4] = \~GND~combout ;

assign gpio9_io_out_en[5] = \~GND~combout ;

assign gpio9_io_out_en[6] = \~GND~combout ;

assign gpio9_io_out_en[7] = \~GND~combout ;

assign resetn_out = ext_resetn;

assign dmactive = \~GND~combout ;

assign swj_JTAGNSW = \~GND~combout ;

assign swj_JTAGSTATE[0] = \~GND~combout ;

assign swj_JTAGSTATE[1] = \~GND~combout ;

assign swj_JTAGSTATE[2] = \~GND~combout ;

assign swj_JTAGSTATE[3] = \~GND~combout ;

assign swj_JTAGIR[0] = \~GND~combout ;

assign swj_JTAGIR[1] = \~GND~combout ;

assign swj_JTAGIR[2] = \~GND~combout ;

assign swj_JTAGIR[3] = \~GND~combout ;

assign ext_dma_DMACCLR[0] = ext_dma_DMACBREQ[0];

assign ext_dma_DMACCLR[1] = ext_dma_DMACBREQ[1];

assign ext_dma_DMACCLR[2] = ext_dma_DMACBREQ[2];

assign ext_dma_DMACCLR[3] = ext_dma_DMACBREQ[3];

assign ext_dma_DMACTC[0] = ext_dma_DMACBREQ[0];

assign ext_dma_DMACTC[1] = ext_dma_DMACBREQ[1];

assign ext_dma_DMACTC[2] = ext_dma_DMACBREQ[2];

assign ext_dma_DMACTC[3] = ext_dma_DMACBREQ[3];

endmodule

module hard_block (
	hbo_22_f9ff3d300b43c0f2_bp,
	hbi_71_0_4730eacd893fc1ea_bp,
	hbo_13_1797ab7b230f061a_bp,
	hbi_272_0_9cb2c0024f9919c5_bp,
	hbi_272_1_9cb2c0024f9919c5_bp,
	hbi_69_0_9cb2c0024f9919c5_bp,
	hbi_7_0_4730eacd893fc1ea_bp,
	devpor,
	devclrn,
	devoe);
output 	hbo_22_f9ff3d300b43c0f2_bp;
input 	hbi_71_0_4730eacd893fc1ea_bp;
output 	hbo_13_1797ab7b230f061a_bp;
input 	hbi_272_0_9cb2c0024f9919c5_bp;
input 	hbi_272_1_9cb2c0024f9919c5_bp;
input 	hbi_69_0_9cb2c0024f9919c5_bp;
input 	hbi_7_0_4730eacd893fc1ea_bp;

// Design Ports Information
// ~ALTERA_ASDO_DATA1~	=>  Location: PIN_F4,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: Default
// ~ALTERA_FLASH_nCE_nCSO~	=>  Location: PIN_E2,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: Default
// ~ALTERA_DCLK~	=>  Location: PIN_P3,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: Default
// ~ALTERA_DATA0~	=>  Location: PIN_N7,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: Default
// ~ALTERA_nCEO~	=>  Location: PIN_P28,	 I/O Standard: 3.3-V LVTTL,	 Current Strength: 8mA

input 	devpor;
input 	devclrn;
input 	devoe;

wire gnd;
wire vcc;
wire unknown;

assign gnd = 1'b0;
assign vcc = 1'b1;
assign unknown = 1'bx;

wire \gclksw_inst|clkout ;
wire \pll_inst|auto_generated|pll1~LOCKED ;
wire \pll_inst|auto_generated|pll1~FBOUT ;
wire [4:0] \pll_inst|auto_generated|clk ;

wire [4:0] \pll_inst|auto_generated|pll1_CLK_bus ;

assign \pll_inst|auto_generated|clk [0] = \pll_inst|auto_generated|pll1_CLK_bus [0];
assign \pll_inst|auto_generated|clk [1] = \pll_inst|auto_generated|pll1_CLK_bus [1];
assign \pll_inst|auto_generated|clk [2] = \pll_inst|auto_generated|pll1_CLK_bus [2];
assign \pll_inst|auto_generated|clk [3] = \pll_inst|auto_generated|pll1_CLK_bus [3];
assign \pll_inst|auto_generated|clk [4] = \pll_inst|auto_generated|pll1_CLK_bus [4];

// Location: CLKCTRL_G3
cycloneive_clkctrl \gclksw_inst|gclk_switch (
	.ena(vcc),
	.inclk({vcc,\pll_inst|auto_generated|clk [0],vcc,hbi_69_0_9cb2c0024f9919c5_bp}),
	.clkselect({hbi_272_1_9cb2c0024f9919c5_bp,hbi_272_0_9cb2c0024f9919c5_bp}),
	.devclrn(devclrn),
	.devpor(devpor),
	.outclk(\gclksw_inst|clkout ));
// synopsys translate_off
defparam \gclksw_inst|gclk_switch .clock_type = "global clock";
defparam \gclksw_inst|gclk_switch .ena_register_mode = "none";
// synopsys translate_on

// Location: PLL_1
cycloneive_pll \pll_inst|auto_generated|pll1 (
	.areset(!hbi_71_0_4730eacd893fc1ea_bp),
	.pfdena(vcc),
	.fbin(\pll_inst|auto_generated|pll1~FBOUT ),
	.phaseupdown(gnd),
	.phasestep(gnd),
	.scandata(gnd),
	.scanclk(gnd),
	.scanclkena(vcc),
	.configupdate(gnd),
	.clkswitch(gnd),
	.inclk({gnd,hbi_7_0_4730eacd893fc1ea_bp}),
	.phasecounterselect(3'b000),
	.phasedone(),
	.scandataout(),
	.scandone(),
	.activeclock(),
	.locked(\pll_inst|auto_generated|pll1~LOCKED ),
	.vcooverrange(),
	.vcounderrange(),
	.fbout(\pll_inst|auto_generated|pll1~FBOUT ),
	.clk(\pll_inst|auto_generated|pll1_CLK_bus ),
	.clkbad());
// synopsys translate_off
defparam \pll_inst|auto_generated|pll1 .auto_settings = "false";
defparam \pll_inst|auto_generated|pll1 .bandwidth_type = "medium";
defparam \pll_inst|auto_generated|pll1 .c0_high = 1;
defparam \pll_inst|auto_generated|pll1 .c0_initial = 1;
defparam \pll_inst|auto_generated|pll1 .c0_low = 1;
defparam \pll_inst|auto_generated|pll1 .c0_mode = "even";
defparam \pll_inst|auto_generated|pll1 .c0_ph = 0;
defparam \pll_inst|auto_generated|pll1 .c1_high = 0;
defparam \pll_inst|auto_generated|pll1 .c1_initial = 0;
defparam \pll_inst|auto_generated|pll1 .c1_low = 0;
defparam \pll_inst|auto_generated|pll1 .c1_mode = "bypass";
defparam \pll_inst|auto_generated|pll1 .c1_ph = 0;
defparam \pll_inst|auto_generated|pll1 .c1_use_casc_in = "off";
defparam \pll_inst|auto_generated|pll1 .c2_high = 0;
defparam \pll_inst|auto_generated|pll1 .c2_initial = 0;
defparam \pll_inst|auto_generated|pll1 .c2_low = 0;
defparam \pll_inst|auto_generated|pll1 .c2_mode = "bypass";
defparam \pll_inst|auto_generated|pll1 .c2_ph = 0;
defparam \pll_inst|auto_generated|pll1 .c2_use_casc_in = "off";
defparam \pll_inst|auto_generated|pll1 .c3_high = 0;
defparam \pll_inst|auto_generated|pll1 .c3_initial = 0;
defparam \pll_inst|auto_generated|pll1 .c3_low = 0;
defparam \pll_inst|auto_generated|pll1 .c3_mode = "bypass";
defparam \pll_inst|auto_generated|pll1 .c3_ph = 0;
defparam \pll_inst|auto_generated|pll1 .c3_use_casc_in = "off";
defparam \pll_inst|auto_generated|pll1 .c4_high = 0;
defparam \pll_inst|auto_generated|pll1 .c4_initial = 0;
defparam \pll_inst|auto_generated|pll1 .c4_low = 0;
defparam \pll_inst|auto_generated|pll1 .c4_mode = "bypass";
defparam \pll_inst|auto_generated|pll1 .c4_ph = 0;
defparam \pll_inst|auto_generated|pll1 .c4_use_casc_in = "off";
defparam \pll_inst|auto_generated|pll1 .charge_pump_current_bits = 1;
defparam \pll_inst|auto_generated|pll1 .clk0_counter = "c0";
defparam \pll_inst|auto_generated|pll1 .clk0_divide_by = 1;
defparam \pll_inst|auto_generated|pll1 .clk0_duty_cycle = 50;
defparam \pll_inst|auto_generated|pll1 .clk0_multiply_by = 30;
defparam \pll_inst|auto_generated|pll1 .clk0_phase_shift = "0";
defparam \pll_inst|auto_generated|pll1 .clk1_counter = "unused";
defparam \pll_inst|auto_generated|pll1 .clk1_divide_by = 0;
defparam \pll_inst|auto_generated|pll1 .clk1_duty_cycle = 50;
defparam \pll_inst|auto_generated|pll1 .clk1_multiply_by = 0;
defparam \pll_inst|auto_generated|pll1 .clk1_phase_shift = "0";
defparam \pll_inst|auto_generated|pll1 .clk2_counter = "unused";
defparam \pll_inst|auto_generated|pll1 .clk2_divide_by = 0;
defparam \pll_inst|auto_generated|pll1 .clk2_duty_cycle = 50;
defparam \pll_inst|auto_generated|pll1 .clk2_multiply_by = 0;
defparam \pll_inst|auto_generated|pll1 .clk2_phase_shift = "0";
defparam \pll_inst|auto_generated|pll1 .clk3_counter = "unused";
defparam \pll_inst|auto_generated|pll1 .clk3_divide_by = 0;
defparam \pll_inst|auto_generated|pll1 .clk3_duty_cycle = 50;
defparam \pll_inst|auto_generated|pll1 .clk3_multiply_by = 0;
defparam \pll_inst|auto_generated|pll1 .clk3_phase_shift = "0";
defparam \pll_inst|auto_generated|pll1 .clk4_counter = "unused";
defparam \pll_inst|auto_generated|pll1 .clk4_divide_by = 0;
defparam \pll_inst|auto_generated|pll1 .clk4_duty_cycle = 50;
defparam \pll_inst|auto_generated|pll1 .clk4_multiply_by = 0;
defparam \pll_inst|auto_generated|pll1 .clk4_phase_shift = "0";
defparam \pll_inst|auto_generated|pll1 .compensate_clock = "clock0";
defparam \pll_inst|auto_generated|pll1 .inclk0_input_frequency = 125000;
defparam \pll_inst|auto_generated|pll1 .inclk1_input_frequency = 0;
defparam \pll_inst|auto_generated|pll1 .loop_filter_c_bits = 0;
defparam \pll_inst|auto_generated|pll1 .loop_filter_r_bits = 19;
defparam \pll_inst|auto_generated|pll1 .m = 60;
defparam \pll_inst|auto_generated|pll1 .m_initial = 1;
defparam \pll_inst|auto_generated|pll1 .m_ph = 0;
defparam \pll_inst|auto_generated|pll1 .n = 1;
defparam \pll_inst|auto_generated|pll1 .operation_mode = "normal";
defparam \pll_inst|auto_generated|pll1 .pfd_max = 200000;
defparam \pll_inst|auto_generated|pll1 .pfd_min = 3076;
defparam \pll_inst|auto_generated|pll1 .pll_compensation_delay = 6547;
defparam \pll_inst|auto_generated|pll1 .self_reset_on_loss_lock = "off";
defparam \pll_inst|auto_generated|pll1 .simulation_type = "timing";
defparam \pll_inst|auto_generated|pll1 .switch_over_type = "auto";
defparam \pll_inst|auto_generated|pll1 .vco_center = 1538;
defparam \pll_inst|auto_generated|pll1 .vco_divide_by = 0;
defparam \pll_inst|auto_generated|pll1 .vco_frequency_control = "auto";
defparam \pll_inst|auto_generated|pll1 .vco_max = 3333;
defparam \pll_inst|auto_generated|pll1 .vco_min = 1538;
defparam \pll_inst|auto_generated|pll1 .vco_multiply_by = 0;
defparam \pll_inst|auto_generated|pll1 .vco_phase_shift_step = 260;
defparam \pll_inst|auto_generated|pll1 .vco_post_scale = 2;
// synopsys translate_on

assign hbo_22_f9ff3d300b43c0f2_bp = \gclksw_inst|clkout ;

assign hbo_13_1797ab7b230f061a_bp = \pll_inst|auto_generated|pll1~LOCKED ;

endmodule
