set_instance_assignment -name ENABLE_OPEN_DRAIN -to GPIO6_2~output false
set_instance_assignment -name ENABLE_OPEN_DRAIN -to GPIO6_0~output false
set_instance_assignment -name ENABLE_OPEN_DRAIN -to GPIO9_1~output false
set_instance_assignment -name ENABLE_OPEN_DRAIN -to GPIO9_2~output false
set_instance_assignment -name ENABLE_OPEN_DRAIN -to GPIO9_0~output false
set_instance_assignment -extension -name CLKIN_FREQ -to pll_inst|auto_generated|pll1 8
set_instance_assignment -extension -name FIXED_COORD -to gclksw_inst|gclk_switch__alta_gclksw {22 4 0}
set_instance_assignment -extension -name FIXED_COORD -to gclksw_inst|gclk_switch {22 4 5}
set_location_assignment -to GPIO3_0 PIN_95
set_location_assignment -to GPIO6_0 PIN_51
set_location_assignment -to GPIO6_2 PIN_52
set_location_assignment -to GPIO9_0 PIN_47
set_location_assignment -to GPIO9_1 PIN_48
set_location_assignment -to GPIO9_2 PIN_46
set_location_assignment -to PIN_HSE PIN_HSE
set_location_assignment -to PIN_HSI PIN_HSI
set_location_assignment -to PIN_OSC PIN_OSC
